[Main]
FileType=CIR
Version=7.00
Program=Micro-Cap
Screen=1280,1024
MCAPVersion=7.0.0.0
Key ID=12 345 678
NLCnt=143
TXCnt=23

[shapedef]
Name=Battery
Line=0,0,22,0
Line=22,-3,22,3
Line=26,-7,26,7
Line=26,0,48,0
Current=32,8,16,8

[shapedef]
Name=Resistor
PolyOpen=12 
PolyLine=0,0
PolyLine=0,0
PolyLine=12,0
PolyLine=14,-4
PolyLine=18,4
PolyLine=22,-4
PolyLine=26,4
PolyLine=30,-4
PolyLine=34,4
PolyLine=36,0
PolyLine=48,0
PolyLine=48,0
Current=32,8,16,8

[shapedef]
Name=Capacitor
Line=0,0,22,0
Line=22,-8,22,8
Line=26,-8,26,8
Line=26,0,48,0
Current=32,12,16,12

[shapedef]
Name=Diode
Root="Diode.root",0,-8,0

[shapedef]
Name=NFV
Root="Vsource.root",0,-12,0
Root="TextNv.Root",20,-6,0
Root="TextFv.Root",20,1,0

[shapedef]
Name=Jnpc
Rectangle=8,-8,72,56
Line=0,0,8,0
Line=0,48,8,48
PolyClosed=3 
PolyLine=8,16
PolyLine=16,24
PolyLine=8,32
Ellipse=38,-12,42,-8
Ellipse=38,56,42,60
Ellipse=72,46,76,50
Ellipse=4,22,8,26
Line=4,24,0,24
Line=76,48,80,48
Line=72,0,80,0
Line=40,60,40,72
Line=40,-12,40,-24

[shapedef]
Name=Opamp5
Root="Opamp.root",0,-4,0
Root="Plus.root",23,-6,0
Root="Minus.root",23,52,0
Line=32,56,32,34
Line=32,-8,32,13

[shapedef]
Name=Ground
Line=0,0,12,0
Line=12,-8,12,8
Line=18,-4,18,4
Line=24,0,24,0

[shapedef]
Name=Switch
Line=0,0,0,0
Line=0,48,0,48
Line=48,0,48,16
Line=48,48,48,24
Line=48,16,52,20
Root="Plus.root",6,6,0
Root="Minus.root",6,40,0
Ellipse=-2,-2,2,2
Ellipse=-2,46,2,50

[shapedef]
Name=Diode.root
Line=0,0,20,0
Line=28,0,48,0
Rectangle=18,-8,20,8,SOLID
PolyClosed=3 ,Solid
PolyLine=20,0
PolyLine=28,-8
PolyLine=28,8
Current=32,16,16,16

[shapedef]
Name=Opamp.root
Line=0,48,6,48
Line=0,0,5,0
Line=6,-4,6,52
Line=6,-4,48,24
Line=6,52,48,24
Line=48,24,72,24
Line=9,10,15,10
Line=12,7,12,13
Line=9,38,15,38
Line=4,0,6,0

[shapedef]
Name=Minus.root
Line=-2,0,2,0

[shapedef]
Name=Vsource.root
Line=0,0,12,0
Line=36,0,48,0
Ellipse=12,-12,36,12
Line=7,5,7,9
Root="Plus.root",39,5,0
Current=32,16,16,16

[shapedef]
Name=Or.root
Line=42,8,48,8
Line=0,0,10,0
Line=0,16,10,16
Line=24,-4,6,-4
Line=6,20,24,20
Arc=5,-4,43,34 , 42,8,24,-4
Arc=0,-4,12,20 , 6,20,6,-4
Arc=5,-18,43,20 , 24,20,42,8

[shapedef]
Name=Plus.root
Line=-2,0,2,0
Line=0,-2,0,2

[shapedef]
Name=Plt.root
Rectangle=16,-24,64,24
Line=0,0,16,0
Line=22,0,57,0
Line=40,-18,40,18
Line=64,0,80,0

[shapedef]
Name=TextNv.Root
Line=0,0,8,0
Line=8,0,0,5
Line=0,5,8,5

[shapedef]
Name=TextFv.Root
Line=0,0,8,0
Line=4,0,4,2
Line=8,0,8,5

[shapedef]
Name=Or4
Root="Bigor.root",0,-20,0
Line=0,0,10,0
Line=0,32,10,32

[shapedef]
Name=Schmitt
Root="Plt.root",0,-24,0
Line=27,-8,48,-8
Line=48,-8,48,8
Line=53,8,32,8
Line=32,8,32,-8

[shapedef]
Name=Bigor.root
Root="Or.root",0,-2,0
Arc=1,-12,11,12 , 6,12,6,-12
Arc=1,36,11,60 , 6,60,6,36

[shapedef]
Name=STIM1
Arc=50,-8,62,8 , 56,8,62,0
Arc=50,-8,62,8 , 62,0,56,-8
Line=13,8,57,8
Arc=8,-8,18,8 , 13,-8,8,0
Ellipse=53,-3,59,3,SOLID
Line=64,0,72,0
Arc=8,-8,18,8 , 8,0,13,8
Line=13,-8,57,-8
Line=56,0,64,0
Line=17,4,22,4
Line=22,4,22,-5
Line=22,-5,29,-5
Line=29,-5,29,4
Line=29,4,33,4
Line=33,4,33,-5
Line=33,-5,36,-5
Line=36,-5,36,4
Line=36,4,41,4
Line=41,4,41,-5
Line=41,-5,43,-5

[shapedef]
Name=LatchSR
Rectangle=-8,-8,56,56
Line=-16,0,-8,0
Ellipse=22,-12,26,-8
Ellipse=22,56,26,60
Ellipse=56,46,60,50
Line=60,48,64,48
Line=-8,24,-16,24
Line=-8,48,-16,48
Line=24,60,24,72
Line=56,0,64,0
Line=24,-12,24,-24

[shapedef]
Name=Fixed
Line=8,0,32,0
Line=8,0,0,-8
Line=8,0,0,8

[compdef]
Name=Battery1
Definition=Battery
Shape=Battery
Mask=5888
Label Offset=0,0,0,0
PinCnt=2
Pin="Plus",6,0,-4,-1
Pin="Minus",0,0,-14,-1

[compdef]
Name=Or4
Definition=OR
Shape=Or4
Mask=4096
Data1=4
Label Offset=14,12,-1,14
PinCnt=5
Pin="In0",0,0,-7,-1
Pin="In1",0,1,-18,8
Pin="In2",0,3,-18,7
Pin="In3",0,4,-7,15
Pin="Out",6,2,-8,-2

[compdef]
Name=Opamp
Definition=Opamp
Shape=Opamp5
Mask=4097
Label Offset=44,29,-14,39
PinCnt=5
Pin="Plus input",0,0,-31,-7
Pin="Minus input",0,6,-33,20
Pin="VEE",4,7,3,-5
Pin="Output",9,3,-13,-4
Pin="VCC",4,-1,5,14

[compdef]
Name=SRFF
Definition=SRFF
Shape=LatchSR
Mask=20483
Data1=1
Label Offset=38,9,-31,41
PinCnt=7
Pin="PREB",3,-3,-13,30
Pin="CLRB",3,9,-14,-17
Pin="GATE",-2,3,12,8
Pin="S",-2,0,12,6
Pin="R",-2,6,12,7
Pin="Q",8,0,-18,6
Pin="QB",8,6,-24,7

[compdef]
Name=Fixed Digital
Definition=DIGITAL STATE
Shape=Fixed
Mask=3072
Label Offset=-14,-7,-6,-27
PinCnt=1
Pin="Out",4,0,-8,-3

[compdef]
Name=Resistor1
Definition=Resistor
Shape=Resistor
Mask=6913
Label Offset=18,6,8,11
PinCnt=2
Pin="Plus",6,0,-10,-4
Pin="Minus",0,0,-14,-4

[compdef]
Name=Ground
Definition=Ground
Shape=Ground
Mask=1793
Label Offset=0,0,0,0
PinCnt=1
Pin="PinA",0,0,-3,-7

[compdef]
Name=JKFF
Definition=JKFF
Shape=Jnpc
Mask=20483
Data1=1
Label Offset=55,9,-29,57
PinCnt=7
Pin="PREB",5,-3,-14,31
Pin="CLRB",5,9,-16,-18
Pin="CLKB",0,3,19,7
Pin="J",0,0,13,7
Pin="K",0,6,12,6
Pin="Q",10,0,-20,7
Pin="QB",10,6,-27,6

[compdef]
Name=Diode1
Definition=Diode
Shape=Diode
Mask=5889
Label Offset=17,10,12,12
PinCnt=2
Pin="Anode",6,0,-9,-8
Pin="Cathode",0,0,-20,-8

[compdef]
Name=Capacitor
Definition=Capacitor
Shape=Capacitor
Mask=6913
Label Offset=19,8,12,12
PinCnt=2
Pin="Plus",6,0,-3,-5
Pin="Minus",0,0,-14,-5

[compdef]
Name=S (V-Switch)
Definition=S
Shape=Switch
Mask=4096
Label Offset=56,9,-27,51
PinCnt=4
Pin="Plus Output",6,0,-3,-3
Pin="Minus Output",6,6,-5,20
Pin="Plus Control",0,0,-33,-3
Pin="Minus Control",0,6,-41,20

[compdef]
Name=NFV
Definition=NFV
Shape=NFV
Mask=4864
Label Offset=18,12,16,13
PinCnt=2
Pin="Plus",6,0,-8,-4
Pin="Minus",0,0,-21,-6

[compdef]
Name=Stim1
Definition=STIM
Shape=STIM1
Mask=5123
Data2=1
Label Offset=-10,-6,13,20
PinCnt=1
Pin="Out0",9,0,-5,-3

[compdef]
Name=Schmitt
Definition=Macro
Shape=Schmitt
Mask=20480
Label Offset=19,25,29,25
PinCnt=2
Pin="PinA",a,0,0,-13,-4
Pin="PinB",a,10,0,-10,-4

[Circuit]
WinBackGround Color=15
Grid Text Color=Height=-12,FStyle=0,Color=1,Name=Arial
Object Default=Height=-15,FStyle=0,Color=4,Name=Arial
Component Color=12
Attribute Text=Height=-12,FStyle=0,Color=2,Name=Arial
Wire Color=2
Select Color=9
Pin Connection=Height=-10,FStyle=0,Color=9,Name=Arial
Select Box Color=4
Node Number=Height=-11,FStyle=0,Color=13,Name=Arial
Node Voltage Color=0
Current=Height=-11,FStyle=0,Color=12,Name=Arial
Power/Condition=Height=-11,FStyle=0,Color=9,Name=Arial
Digital Path Color=9
Title Block=Height=-15,FStyle=0,Color=0,Name=Arial
Digital 0 Color=0
Digital R Color=11
Digital F Color=11
Digital 1 Color=9
Digital X Color=7
Digital Z Color=8
Window Placement=2,3, -1,-1, -6,-25, 88,88,1078,702
Window Placement in Analysis=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Block Select Color=41
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=$time
TitleBlock One Title=True
Title_Block_Border=False
Title_Block=False

[Wire]
Grids=15,15,81,15

[Comp]
Name=Battery1
Grid=29,106
Rot=3

[Attr]
ONV=-24,-43,PART,V1
Style=8192

[Attr]
ONV=-24,-28,VALUE,5.1
Style=8192

[Comp]
Name=Or4
Grid=114,32

[Attr]
ONV=14,12,PART,U2
Style=8192

[Attr]
ONV=14,27,TIMING MODEL,DLY_TTL

[Attr]
ONV=14,42,I/O MODEL,IO_STD

[Attr]
ONV=14,57,MNTYMXDLY,0

[Attr]
ONV=14,72,IO_LEVEL,0

[Attr]
ONV=14,87,POWER NODE,$G_DPWR

[Attr]
ONV=14,102,GROUND NODE,$G_DGND

[Comp]
Name=Opamp
Grid=25,99
Rot=4

[Attr]
ONV=44,-44,PART,X3
Style=8192

[Attr]
ONV=44,-59,MODEL,OPAMPDC
Style=8192

[Wire]
Grids=15,57,29,57

[Comp]
Name=SRFF
Style=ShowPinText
Grid=65,37

[Attr]
ONV=-16,-28,PART,U3
Style=8192

[Attr]
ONV=38,24,TIMING MODEL,DLY_GFF

[Attr]
ONV=38,39,I/O MODEL,IO_STD

[Attr]
ONV=38,54,MNTYMXDLY,0

[Attr]
ONV=38,69,IO_LEVEL,0

[Attr]
ONV=38,84,POWER NODE,$G_DPWR

[Attr]
ONV=38,99,GROUND NODE,$G_DGND

[Wire]
Grids=46,37,49,37

[Comp]
Name=Fixed Digital
Grid=57,40
Rot=4

[Attr]
ONV=-14,-8,PART,U4

[Attr]
ONV=-14,-23,VALUE,1
Style=8192

[Attr]
ONV=-14,-38,I/O MODEL,IO_STD

[Attr]
ONV=-14,-53,IO_LEVEL,0

[Attr]
ONV=-14,-68,POWER NODE,$G_DPWR

[Attr]
ONV=-14,-83,GROUND NODE,$G_DGND

[Comp]
Name=Resistor1
Grid=29,64
Rot=7

[Attr]
ONV=-24,11,PART,R3
Style=8192

[Attr]
ONV=-27,26,VALUE,300
Style=8192

[Wire]
Grids=29,57,29,64

[Wire]
Grids=29,70,29,73

[Wire]
Grids=29,79,29,87

[Comp]
Name=Ground
Grid=35,79
Rot=7

[Wire]
Grids=77,37,77,73

[Comp]
Name=JKFF
Style=ShowPinText
Grid=95,43

[Attr]
ONV=1,-24,PART,U5
Style=8192

[Attr]
ONV=55,24,TIMING MODEL,T_JKFF

[Attr]
ONV=55,39,I/O MODEL,IO_STD

[Attr]
ONV=55,54,MNTYMXDLY,0

[Attr]
ONV=55,69,IO_LEVEL,0

[Attr]
ONV=55,84,POWER NODE,$G_DPWR

[Attr]
ONV=55,99,GROUND NODE,$G_DGND

[Wire]
Grids=92,43,95,43

[Wire]
Grids=92,43,92,49

[Wire]
Grids=92,49,95,49

[Comp]
Name=Fixed Digital
Grid=88,43
Rot=4

[Attr]
ONV=-14,-8,PART,U6

[Attr]
ONV=-14,-23,VALUE,1
Style=8192

[Attr]
ONV=-14,-38,I/O MODEL,IO_STD

[Attr]
ONV=-14,-53,IO_LEVEL,0

[Attr]
ONV=-14,-68,POWER NODE,$G_DPWR

[Attr]
ONV=-14,-83,GROUND NODE,$G_DGND

[Wire]
Grids=77,37,107,37

[Wire]
Grids=107,33,107,37

[Wire]
Grids=107,33,114,33

[Wire]
Grids=105,43,108,43

[Wire]
Grids=110,35,114,35

[Comp]
Name=SRFF
Style=ShowPinText
Grid=97,73

[Attr]
ONV=-14,-27,PART,U7
Style=8192

[Attr]
ONV=38,24,TIMING MODEL,DLY_GFF

[Attr]
ONV=38,39,I/O MODEL,IO_STD

[Attr]
ONV=38,54,MNTYMXDLY,0

[Attr]
ONV=38,69,IO_LEVEL,0

[Attr]
ONV=38,84,POWER NODE,$G_DPWR

[Attr]
ONV=38,99,GROUND NODE,$G_DGND

[Comp]
Name=Fixed Digital
Grid=88,76
Rot=4

[Attr]
ONV=-14,-8,PART,U8

[Attr]
ONV=-14,-23,VALUE,1
Style=8192

[Attr]
ONV=-14,-38,I/O MODEL,IO_STD

[Attr]
ONV=-14,-53,IO_LEVEL,0

[Attr]
ONV=-14,-68,POWER NODE,$G_DPWR

[Attr]
ONV=-14,-83,GROUND NODE,$G_DGND

[Wire]
Grids=77,73,95,73

[Wire]
Grids=113,36,114,36

[Wire]
Grids=34,96,47,96

[Wire]
Grids=47,96,47,117

[Comp]
Name=Diode1
Grid=54,96
Rot=2

[Attr]
ONV=-33,-25,PART,D2
Style=8192

[Attr]
ONV=-44,11,MODEL,1n4148
Style=8192

[Comp]
Name=Diode1
Grid=60,96
Rot=2

[Attr]
ONV=-33,-25,PART,D3
Style=8192

[Attr]
ONV=-43,11,MODEL,1n4148
Style=8192

[Comp]
Name=Resistor1
Grid=60,96

[Attr]
ONV=21,-22,PART,R5
Style=8192

[Attr]
ONV=17,10,VALUE,10K
Style=8192

[Comp]
Name=Resistor1
Grid=68,98
Rot=1

[Attr]
ONV=8,11,PART,R6
Style=8192

[Attr]
ONV=8,26,VALUE,5K
Style=8192

[Wire]
Grids=66,96,68,96

[Wire]
Grids=68,96,76,96

[Wire]
Grids=14,117,47,117

[Wire]
Grids=95,79,95,99

[Comp]
Name=Resistor1
Grid=133,34
Rot=2

[Attr]
ONV=-34,-21,PART,R7
Style=8192

[Attr]
ONV=-35,8,VALUE,100
Style=8192

[Comp]
Name=Resistor1
Grid=142,48
Rot=3

[Attr]
ONV=-24,-26,PART,R8
Style=8192

[Attr]
ONV=-34,-10,VALUE,1Meg
Style=8192

[Wire]
Grids=133,34,142,34

[Wire]
Grids=142,34,142,42

[Comp]
Name=Capacitor
Grid=148,42
Rot=7

[Attr]
ONV=13,10,PART,C2
Style=8192

[Attr]
ONV=10,32,VALUE,500p
Style=8192

[Comp]
Name=S (V-Switch)
Grid=158,36

[Attr]
ONV=56,9,PART,S2
Style=8192

[Attr]
ONV=56,24,MODEL,SW2OFF
Style=8192

[Comp]
Name=S (V-Switch)
Grid=158,50

[Attr]
ONV=56,9,PART,S3
Style=8192

[Attr]
ONV=56,24,MODEL,SW2ON
Style=8192

[Comp]
Name=S (V-Switch)
Grid=35,73
Rot=6

[Attr]
ONV=-71,9,PART,S4
Style=8192

[Attr]
ONV=12,19,MODEL,SW2ON
Style=8192

[Wire]
Grids=148,56,158,56

[Wire]
Grids=148,34,148,42

[Wire]
Grids=142,34,148,34

[Wire]
Grids=148,48,148,56

[Wire]
Grids=142,48,142,56

[Wire]
Grids=142,56,148,56

[Wire]
Grids=164,56,174,56

[Wire]
Grids=164,45,174,45

[Comp]
Name=Diode1
Grid=164,34
Rot=5

[Attr]
ONV=12,-27,PART,D5
Style=8192

[Attr]
ONV=12,-42,MODEL,1N4148
Style=8192

[Wire]
Grids=164,42,164,45

[Comp]
Name=Ground
Grid=158,42
Rot=7

[Wire]
Grids=164,45,164,50

[Wire]
Grids=158,34,158,36

[Wire]
Grids=148,34,155,34

[Wire]
Grids=164,34,164,36

[Wire]
Grids=155,50,158,50

[Wire]
Grids=155,34,155,50

[Wire]
Grids=155,34,158,34

[Comp]
Name=Ground
Grid=158,56
Rot=7

[Wire]
Grids=14,93,25,93

[Wire]
Grids=15,29,23,29

[Comp]
Name=NFV
Grid=22,105
Rot=3

[Attr]
ONV=-31,-28,PART,E4
Style=8192

[Attr]
ONV=-136,-13,VALUE,.5*(V(VREF)-V(GND))
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Wire]
Grids=105,79,113,79

[Wire]
Grids=113,36,113,79

[Wire]
Grids=29,87,42,87

[Comp]
Name=Stim1
Grid=86,65
Rot=4

[Attr]
ONV=-10,-9,PART,U9
Style=8192
Color=9

[Attr]
ONV=-10,-24,FORMAT,1
Color=9

[Attr]
ONV=-10,-39,COMMAND,PATTERN1
Color=9

[Attr]
ONV=-10,-54,I/O MODEL,IO_STD
Color=9

[Attr]
ONV=-10,-69,TIMESTEP,0
Color=9

[Attr]
ONV=-10,-84,IO_LEVEL,0
Color=9

[Attr]
ONV=-10,-99,POWER NODE,$G_DPWR
Color=9

[Attr]
ONV=-10,-114,GROUND NODE,$G_DGND
Color=9

[Attr]
ONV=0,99,COST,
Color=9

[Attr]
ONV=0,110,POWER,
Color=9

[Wire]
Grids=68,34,89,34

[Wire]
Grids=100,34,100,40

[Wire]
Grids=83,46,95,46

[Wire]
Grids=73,37,77,37

[Wire]
Grids=61,40,61,46

[Wire]
Grids=61,46,68,46

[Wire]
Grids=92,49,92,52

[Wire]
Grids=92,52,100,52

[Wire]
Grids=92,76,92,82

[Wire]
Grids=92,82,100,82

[Wire]
Grids=92,76,95,76

[Wire]
Grids=100,65,100,70

[Wire]
Grids=95,65,100,65

[Wire]
Grids=61,40,63,40

[Comp]
Name=Diode1
Grid=76,98
Rot=7

[Attr]
ONV=5,2,PART,D7
Style=8192

[Attr]
ONV=6,33,MODEL,DZ1
Style=8192

[Comp]
Name=Schmitt
Style=ShowPinText
Grid=81,15

[Attr]
ONV=19,25,PART,X6
Style=8192
Color=9

[Attr]
ONV=19,40,FILE,SCHMITT
Style=8192
Color=9

[Attr]
ONV=19,55,Param:X1,{VOFF}
Style=12288
Color=9

[Attr]
ONV=19,70,Param:X2,{VON}
Style=12288
Color=9

[Attr]
ONV=19,85,Param:Y1,0
Style=12288
Color=9

[Attr]
ONV=18,100,Param:Y2,1
Style=12288
Color=9

[Attr]
ONV=19,115,Param:Rout,1
Color=9

[Attr]
ONV=19,130,Param:Sign,1
Color=9

[Wire]
Grids=114,15,114,19

[Wire]
Grids=91,15,114,15

[Wire]
Grids=35,73,77,73

[Wire]
Grids=29,87,29,92

[Wire]
Grids=47,96,48,96

[Wire]
Grids=68,96,68,98

[Wire]
Grids=76,96,76,98

[Wire]
Grids=68,104,68,107

[Wire]
Grids=76,104,76,107

[Wire]
Grids=68,107,76,107

[Wire]
Grids=22,107,29,107

[Wire]
Grids=42,87,42,107

[Wire]
Grids=42,107,68,107

[Comp]
Name=NFV
Grid=23,35
Rot=3

[Attr]
ONV=-31,-28,PART,E5
Style=8192

[Attr]
ONV=-66,21,VALUE,LIMIT(5*(V(GOOD)),0,5)
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Wire]
Grids=23,35,23,36

[Wire]
Grids=23,36,27,36

[Comp]
Name=NFV
Grid=38,59
Rot=3

[Attr]
ONV=-31,-28,PART,E6
Style=8192

[Attr]
ONV=-45,26,VALUE,IF(V(RTCT)>.8,0,2)
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=48,59
Rot=7

[Comp]
Name=Ground
Grid=38,59
Rot=7

[Comp]
Name=Capacitor
Grid=48,59
Rot=3

[Attr]
ONV=15,-42,PART,C3
Style=8192

[Attr]
ONV=12,-26,VALUE,1N
Style=8192

[Comp]
Name=Resistor1
Grid=46,53
Rot=2

[Attr]
ONV=-34,-21,PART,R9
Style=8192

[Attr]
ONV=-35,8,VALUE,1K
Style=8192

[Wire]
Grids=38,53,40,53

[Comp]
Name=NFV
Grid=38,43
Rot=3

[Attr]
ONV=-31,-28,PART,E7
Style=8192

[Attr]
ONV=-56,25,VALUE,IF(V(RTCT)>2.5,2,0)
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=38,43
Rot=7

[Comp]
Name=Ground
Grid=49,43
Rot=7

[Comp]
Name=Capacitor
Grid=49,43
Rot=3

[Attr]
ONV=15,-42,PART,C4
Style=8192

[Attr]
ONV=9,-25,VALUE,1N
Style=8192

[Comp]
Name=Resistor1
Grid=46,37
Rot=2

[Attr]
ONV=-34,-21,PART,R10
Style=8192

[Attr]
ONV=-31,9,VALUE,1K
Style=8192

[Wire]
Grids=38,37,40,37

[Wire]
Grids=49,37,63,37

[Wire]
Grids=46,53,48,53

[Wire]
Grids=56,43,63,43

[Wire]
Grids=56,43,56,53

[Wire]
Grids=48,53,56,53

[Comp]
Name=NFV
Grid=85,105
Rot=3

[Attr]
ONV=-31,-28,PART,E8
Style=8192

[Attr]
ONV=-58,28,VALUE,IF(V(ISENSE)>V(A),2,0)
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=95,105
Rot=7

[Comp]
Name=Ground
Grid=85,105
Rot=7

[Comp]
Name=Capacitor
Grid=95,105
Rot=3

[Attr]
ONV=15,-43,PART,C5
Style=8192

[Attr]
ONV=19,-26,VALUE,1N
Style=8192

[Comp]
Name=Resistor1
Grid=93,99
Rot=2

[Attr]
ONV=-34,-21,PART,R11
Style=8192

[Attr]
ONV=-33,9,VALUE,1K
Style=8192

[Wire]
Grids=126,107,160,107

[Wire]
Grids=29,106,29,107

[Wire]
Grids=29,107,34,107

[Wire]
Grids=22,99,25,99

[Wire]
Grids=22,105,22,107

[Wire]
Grids=120,34,126,34

[Wire]
Grids=110,35,110,43

[Wire]
Grids=85,99,87,99

[Wire]
Grids=93,99,95,99

[Wire]
Grids=73,43,83,43

[Wire]
Grids=83,43,83,46

[Wire]
Grids=27,36,29,36

[Wire]
Grids=89,34,100,34

[Wire]
Grids=114,19,114,32

[Wire]
Grids=126,34,127,34

[Wire]
Grids=108,43,110,43

[Wire]
Grids=34,107,42,107

[Node Offsets]
Offset=7,0,120,34,6,-38

[Condition Offsets]

[Grid Text]
Text=Y
Grid=142,34

[Grid Text]
Text=X
Grid=126,34

[Grid Text]
Text=A
Grid=76,96

[Grid Text]
Text="Y"
Grid=59,52

[Grid Text]
Text=GOOD
Grid=114,19

[Grid Text]
Text=TFF
Grid=108,43

[Grid Text]
Text=.PARAMETERS(VOFF=7.6,VON=8.4)
Grid=56,22

[Grid Text]
Text=RESET
Grid=95,65

[Grid Text]
Text=VREF
Grid=15,29
Color=9

[Grid Text]
Text=GND
Grid=27,36

[Grid Text]
Text=VCC
Grid=15,15
Color=9

[Grid Text]
Text=RTCT
Grid=15,57
Color=9

[Grid Text]
Text=COMP
Grid=14,117
Color=9

[Grid Text]
Text=GND
Grid=174,56
Color=9

[Grid Text]
Text=OUT
Grid=174,45
Color=9

[Grid Text]
Text=VFB
Grid=14,93
Color=9

[Grid Text]
Text=ISENSE
Grid=160,107
Color=9

[Grid Text]
Text=VCC
Grid=164,28

[Grid Text]
Text=GND
Grid=34,107

[Grid Text]
Text=V5G
Grid=29,100

[Grid Text]
Text=RESET
Grid=89,34

[Grid Text]
Text="Called by other circuits.  Not intended for stand alone analysis."
Grid=34,7
Height=-19
Color=9

[Grid Text]
Text="PWM_T MACRO"
Grid=61,4
Height=-19
Color=13

[Schematic]
Page 0=0
TabSize 0=320
Page 1=0
TabSize 1=320
Page 2=0
TabSize 2=320
Page 3=0
TabSize 3=320
Splitter.xs=0
Splitter.ys=0
TextQuad=4099
Scale=1
PrinterScale=1
View=304

[Tools]
Pos=Top
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
FLAG=Yes
META=No
INFO=Yes
HELP=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=Yes
GRID=Yes
BORDER=Yes
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FILPX=Yes
FINDCOMP=Yes
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
TOFRONT=Yes
TOBACK=Yes
PAGEADD=Yes
PAGEDEL=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=Yes
COLOR=Yes
FONT=Yes

[Page]
Index=0
Name=Page 1
Scale 0=1
Scale 1=1
Scale 2=1
SB 3=58,93
Scale 3=1
Grid=61,21

[Page]
Index=1
Name=Text
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=2
Name=Models
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=3
Name=Info
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Text Area]
Font=Height=-15,FStyle=0,Color=4,Name=Courier New
Comment Color=8
Background Color=15
Len=2144
*** From file C:\MC8\library\DIGIO.LIB
.MODEL DLY_TTL UGATE (TPLHTY=11NS TPLHMX=22NS TPHLTY=8NS TPHLMX=15NS)

*** From file C:\MC8\library\DIGIO.LIB
.MODEL IO_STD UIO (
+  DRVH=130 DRVL=130
+  ATOD1="ATOD_STD" ATOD2="ATOD_STD_NX"
+  ATOD3="ATOD_STD" ATOD4="ATOD_STD_NX"
+  DTOA1="DTOA_STD" DTOA2="DTOA_STD"
+  DTOA3="DTOA_STD" DTOA4="DTOA_STD"
+  TSWHL1=3.310NS TSWHL2=3.310NS
+  TSWHL3=3.310NS TSWHL4=3.310NS
+  TSWLH1=2.115NS TSWLH2=2.115NS
+  TSWLH3=2.115NS TSWLH4=2.115NS
+  DIGPOWER="DIGIFPWR")

*** From file C:\MC8\library\DIGIO.LIB
.MODEL DLY_GFF UGFF (TPPCQLHTY=16NS TPPCQLHMX=25NS TPPCQHLTY=25NS
+     TPPCQHLMX=40NS TWPCLMN=25NS TPGQLHTY=16NS TPGQLHMX=25NS
+     TPGQHLTY=25NS TPGQHLMX=40NS TWGHMN=30NS TSUDGMN=15NS
+     TSUPCGHMN=10NS THDGMN=5NS)

*** From file C:\MC8\library\ANALOG.LIB
.MODEL T_JKFF UEFF ( 
+ TPCLKQLHMN=2NS TPCLKQLHTY=2NS TPCLKQLHMX=2NS 
+ TPCLKQHLMN=2NS TPCLKQHLTY=2NS TPCLKQHLMX=2NS)

*** From file C:\MC8\library\DIODE.LBR
*** Generic Diode
.MODEL 1N4148 D (IS=6.65129N N=1.93262 BV=100 RS=507.42M TT=1.12599N
+ CJO=1.33719P VJ=8.77381 M=300M RL=3.34895G)

*** From file C:\MC8\library\DIGIO.LIB
.MODEL DO74_NX DOUTPUT (
+  S0NAME="0"  S0VLO=-1.5  S0VHI=1.4
+  S1NAME="1"  S1VLO=1.4   S1VHI=5.5)

*** From file C:\MC8\library\DIGIO.LIB
.MODEL Q74 NPN (ISE=1E-16 ISC=4E-16 BF=49 BR=.33 CJE=1P CJC=.5P VJE=.9
+        VJC=.8 MJE=.5 MJC=.33 TF=.2N TR=10N CJS=3P VJS=.7
+        RC=40 MJS=.33)

*** From file C:\MC8\library\DIGIO.LIB
.MODEL D74CLMP D (IS=1E-14 CJO=5P M=.5 RS=0)

*** From file C:\MC8\library\DIGIO.LIB
.MODEL D74 D (IS=1E-14 CJO=5P M=.5)

*** From file C:\MC8\library\DIGIO.LIB
.MODEL DIN74 DINPUT (
+  S0NAME="0"  S0TSW=3.5NS  S0RLO=7.1   S0RHI=170   ;@6.8 OHMS, .2V
+  S1NAME="1"  S1TSW=7.5NS  S1RLO=415   S1RHI=195   ;@133 OHMS, 3.4V
+  S2NAME="F"  S2TSW=3.5NS  S2RLO=41.8  S2RHI=107   ;@30.1 OHMS, 1.4V
+  S3NAME="R"  S3TSW=3.5NS  S3RLO=41.8  S3RHI=107   ;@30.1 OHMS, 1.4V
+  S4NAME="X"  S4TSW=3.5NS  S4RLO=41.8  S4RHI=107   ;@30.1 OHMS, 1.4V
+  S5NAME="Z"  S5TSW=3.5NS  S5RLO=1MEG  S5RHI=1MEG)

.define PATTERN1
+0NS  0
+50NS 1



[Printer]
T.AutoTile=No
T.BlackBorder=No
A.AutoTile=No
A.BlackBorder=No
D.AutoTile=No
D.BlackBorder=No

[TRANSIENT]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[AC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[DC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[Analysis]
Window Placement=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Num Out Header Left
Num Out Header Center=$MC\n$user\n$company\n$Analysis of $name\n
Num Out Header Right
Num Out Delimiter=32
Analysis Text=Height=-15,FStyle=0,Color=12,Name=Arial
Analysis Grid Color=8
Analysis Graph Background=15
Object Default=Height=-15,FStyle=0,Color=4,Name=Arial
Analysis Window Background=15
NumOut=Height=-15,FStyle=0,Color=4,Name=Courier New
ScaleColor=On
Select Color=9
Select Box Color=4
Cursor Select Color Primary=7
Cursor Select Color Secondary=9
Tracker Intercept=False
Tracker Mouse=True
Tracker Cursor=True
Tracker Foreground=Height=-15,FStyle=0,Color=0,Name=Arial
Tracker Background=11
Data Point Labels Color Fore=Height=-15,FStyle=0,Color=0,Name=Arial
Data Point Labels Color Back=11
AnimateWait=0
AnimateWaitTime=500
Same Y Scales=Yes
T.Save_For_Future=No
A.Save_For_Future=No
D.Save_For_Future=No
T.Reduce_Display=1
T.Reduce_Save=1
A.Reduce_Display=1
A.Reduce_Save=1
D.Reduce_Display=1
D.Reduce_Save=1

[Tools]
Pos=Top
SELECT=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
POLYCLOS=No
SCALE=Yes
CURSOR=Yes
MEASUREH=Yes
MEASUREV=Yes
TAG=Yes
TEXT=Yes
PROPERTY=Yes
START=Yes
STOP=Yes
PAUSE=Yes
DATAPTS=Yes
TOKENS=Yes
RULER=Yes
PLUS=Yes
XAXIS=Yes
YAXIS=Yes
MINORLOG=Yes
BASELINE=Yes
HORIZCUR=Yes
GOTOX=Yes
GOTOY=Yes
GOTOPERF=Yes
GOTOBRNC=Yes
NEXT=Yes
NEXTIN=Yes
PEAK=Yes
VALLEY=Yes
HIGH=Yes
LOW=Yes
INFLECTN=Yes
GHIGH=Yes
GLOW=Yes
BOTTOM=Yes
TOP=Yes
AOUTPUT=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
COLOR=Yes
FONT=Yes

[Monte Carlo Options]
Analysis=Transient
Status=Off
Distribution=Normal
Number of Runs=10

[Monte Carlo Options]
Analysis=AC
Status=Off
Distribution=Normal
Number of Runs=10

[Monte Carlo Options]
Analysis=DC
Status=Off
Distribution=Normal
Number of Runs=10

[Limits]
Analysis=Transient
OPT=120
Horizontal Cursor=False
Temperature Type=Linear

[Limits]
Analysis=AC
OPT=0
Horizontal Cursor=False
Temperature Type=Linear

[Limits]
Analysis=DC
OPT=0
Horizontal Cursor=False
Temperature Type=Linear
Sweep1 type=Auto
Sweep2 type=None

[Optimize]
Format=3

[Optimize]
Analysis=Transient
Method=Standard_Powell

[Optimize]
Analysis=AC
Method=Standard_Powell

[Optimize]
Analysis=DC
Method=Standard_Powell

[Watch]
Format=3

[Watch]
Analysis=Transient
ExprPercentWidth=80

[Watch]
Analysis=AC
ExprPercentWidth=80

[Watch]
Analysis=DC
ExprPercentWidth=80

[DSP]
T.Status=Off
A.Status=Off

[TF]
Input Source
Place Text=False

[SENS]
Multiple=False
Parameter Type=Component
