[Main]
FileType=CIR
Version=7.00
Program=Micro-Cap
Screen=800,600
MCAPVersion=7.0.0.0
Key ID=493 834 421
NLCnt=13
TXCnt=12

[shapedef]
Name=Resistor
PolyOpen=12 
PolyLine=0,0
PolyLine=0,0
PolyLine=12,0
PolyLine=14,-4
PolyLine=18,4
PolyLine=22,-4
PolyLine=26,4
PolyLine=30,-4
PolyLine=34,4
PolyLine=36,0
PolyLine=48,0
PolyLine=48,0
Current=32,8,16,8

[shapedef]
Name=Inductor
Line=42,0,48,0
Line=0,0,5,0
Arc=5,-7,17,7 , 11,-7,5,0
Arc=13,-7,25,7 , 19,-7,13,0
Arc=29,-7,41,7 , 35,-7,29,0
Arc=21,-7,33,7 , 27,-7,21,0
Arc=6,-7,18,7 , 18,0,12,-7
Arc=14,-7,26,7 , 26,0,20,-7
Arc=22,-7,34,7 , 34,0,28,-7
Arc=30,-7,42,7 , 42,0,36,-7
Line=11,-7,12,-7
Line=19,-7,20,-7
Line=27,-7,28,-7
Line=35,-7,36,-7
Arc=13,-4,17,2 , 13,-1,15,2
Arc=29,-4,33,2 , 29,-1,31,2
Arc=21,-4,25,2 , 21,-1,23,2
Arc=14,-4,18,2 , 16,2,18,-1
Arc=30,-4,34,2 , 32,2,34,-1
Arc=22,-4,26,2 , 24,2,26,-1
Line=15,2,16,2
Line=23,2,24,2
Line=31,2,32,2
Line=5,5,9,5
Line=41,5,41,9
Line=39,7,43,7
Current=32,8,16,8

[shapedef]
Name=VOFV
Root="VOFV.Root",-2,-2,0

[shapedef]
Name=Minus.root
Line=-2,0,2,0

[shapedef]
Name=Plus.root
Line=-2,0,2,0
Line=0,-2,0,2

[shapedef]
Name=Vsrc.root
Root="Plus.root",41,6,0
Root="Minus.root",41,40,0
Line=48,0,48,12
Line=48,36,48,48
Ellipse=36,12,61,36
Current=64,16,64,32

[shapedef]
Name=OFV.Root
Root="Plus.root",6,6,0
Ellipse=-2,-2,2,2
Ellipse=-2,46,2,50

[shapedef]
Name=VOFV.Root
Line=0,0,0,0
Line=0,48,0,48
Root="Vsrc.root",36,0,0
Root="OFV.Root",-2,-2,0
Current=64,16,64,32

[shapedef]
Name=Kshape
Line=0,16,4,16
Line=8,16,12,16
Line=16,16,20,16
Line=24,16,28,16
Line=32,16,36,16
Line=40,16,44,16
Line=15,12,19,12
Line=24,12,28,12
Line=32,12,36,12
Arc=0,4,8,12 , 0,8,4,12
Line=8,12,12,12
Arc=36,4,44,12 , 40,12,44,8
Arc=0,20,8,28 , 4,20,0,24
Arc=36,20,44,28 , 44,24,40,20
Line=8,20,12,20
Line=16,20,20,20
Line=24,20,28,20
Line=32,20,36,20

[compdef]
Name=Inductor
Definition=Inductor
Shape=Inductor
Mask=6913
Label Offset=18,3,11,12
PinCnt=2
Pin="Plus",6,0,-5,-9
Pin="Minus",0,0,-3,-9

[compdef]
Name=K
Definition=K
Shape=Kshape
Mask=4352
Label Offset=16,27,-4,12
PinCnt=0

[compdef]
Name=Resistor
Definition=Resistor
Shape=Resistor
Mask=7681
Label Offset=18,6,8,11
PinCnt=2
Pin="Plus",6,0,-10,-4
Pin="Minus",0,0,-14,-4

[compdef]
Name=VofV
Definition=VofV
Shape=VOFV
Mask=4096
Label Offset=62,11,-30,59
PinCnt=4
Pin="Plus Output",6,0,-18,-3
Pin="Minus Output",6,6,-9,18
Pin="Plus Input",0,0,-31,-3
Pin="Minus Input",0,6,-29,18

[Circuit]
WinBackGround Color=15
Grid Text Color=Height=-12,FStyle=0,Color=9,Name=Arial
Object Default=Height=-16,FStyle=0,Color=4,Name=Arial
Component Color=12
Attribute Text=Height=-12,FStyle=0,Color=2,Name=Arial
Wire Color=2
Select Color=9
Pin Color=9
Select Box Color=4
Node Number=Height=-12,FStyle=0,Color=13,Name=Arial
Node Voltage Color=0
Current=Height=-11,FStyle=0,Color=12,Name=Arial
Power/Condition=Height=-11,FStyle=0,Color=9,Name=Arial
Digital Path Color=9
Title Block=Height=-16,FStyle=0,Color=0,Name=Arial
Digital 0 Color=0
Digital R Color=11
Digital F Color=11
Digital 1 Color=9
Digital X Color=7
Digital Z Color=8
Window Placement=2,3, -1,-1, -6,-25, 88,88,730,434
Window Placement in Analysis=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Block Select Color=41
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=Page $page of $maxpage
TitleBlock One Title=True
Title_Block_Border=False
Title_Block=False

[Comp]
Name=Inductor
Grid=22,25
Rot=5

[Attr]
ONV=11,-27,PART,LP
Style=8192

[Attr]
ONV=9,-41,VALUE,(RS/2)/(2*PI*FL)
Style=8192

[Wire]
Grids=7,25,22,25

[Comp]
Name=Inductor
Grid=37,25
Rot=5

[Attr]
ONV=11,-27,PART,LS
Style=8192

[Attr]
ONV=11,-42,VALUE,n*n*(RS/2)/(2*PI*FL)
Style=8192

[Wire]
Grids=37,19,53,19

[Wire]
Grids=37,25,53,25

[Wire]
Grids=53,19,63,19

[Wire]
Grids=53,25,63,25

[Comp]
Name=K
Grid=33,27
Rot=2

[Attr]
ONV=-31,-42,PART,K1
Style=8192

[Attr]
ONV=-49,-57,INDUCTORS,LP LS

[Attr]
ONV=-31,-72,COUPLING,K1

[Comp]
Name=Resistor
Grid=10,19

[Attr]
ONV=18,6,PART,R1
Style=8192

[Attr]
ONV=18,21,VALUE,RS
Style=8192

[Wire]
Grids=7,19,10,19

[Wire]
Grids=16,19,22,19

[Comp]
Name=Resistor
Grid=53,19
Rot=1

[Attr]
ONV=8,11,PART,R2
Style=8192

[Attr]
ONV=8,26,VALUE,n*n*RS
Style=8192

[Comp]
Name=VofV
Grid=63,19

[Attr]
ONV=62,11,PART,E1
Style=8192

[Attr]
ONV=110,13,VALUE,2*(RS+n*n*RS)/(n*n*RS)
Style=8192

[Node Offsets]

[Condition Offsets]

[Grid Text]
Text=.HELP RS "Primary series resistance"
Grid=22,36

[Grid Text]
Text=.parameters(RS=10,N=1,FL=1k,FH=10Meg)
Grid=21,16
Color=12

[Grid Text]
Text=.define k1 sqrt(1/(1+4*(FL/FH)))
Grid=22,30

[Grid Text]
Text=Outm
Grid=69,25

[Grid Text]
Text=Outp
Grid=69,19

[Grid Text]
Text=Inm
Grid=7,25

[Grid Text]
Text=Inp
Grid=7,19

[Grid Text]
Text=Called by other circuits.  Not intended for stand alone analysis.
Grid=5,10
Height=-19

[Grid Text]
Text=WIDEBAND MACRO
Grid=5,6
Height=-19
Color=13

[Grid Text]
Text=.HELP N "Number of turns"
Grid=22,38

[Grid Text]
Text=.HELP FL "Low frequency breakpoint"
Grid=22,40

[Grid Text]
Text=.HELP FH "HIgh frequency breakpoint"
Grid=22,42

[Schematic]
Page 0=0
TabSize 0=320
Page 1=0
TabSize 1=320
Page 2=0
TabSize 2=320
Page 3=0
TabSize 3=320
Splitter.xs=0
Splitter.ys=0
TextQuad=4099
Scale=0.6666666666666666
PrinterScale=1
View=304

[Tools]
Pos=Top
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
FLAG=No
META=No
INFO=Yes
HELP=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=No
GRID=Yes
BORDER=No
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FILPX=Yes
FINDCOMP=No
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
TOFRONT=No
TOBACK=No
PAGEADD=No
PAGEDEL=No
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=No
COLOR=Yes
FONT=Yes

[Page]
Index=0
Name=Page 1
Scale 0=0.6666666666666666
Scale 1=1
Scale 2=1
Scale 3=1
Grid=66,37

[Text Area]
Font=Height=-13,FStyle=0,Color=4,Name=Courier New
Comment Color=8
Background Color=15
Len=91
03/05/2001 Added gain stage to output to compensate for gain loss due to the two resistors.

[Printer]
T.AutoTile=No
T.BlackBorder=No
A.AutoTile=No
A.BlackBorder=No
D.AutoTile=No
D.BlackBorder=No

[TRANSIENT]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[AC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[DC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[Analysis]
Window Placement=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Num Out Header Left
Num Out Header Center=$MC\n$user\n$company\n$Analysis of $name\n
Num Out Header Right
Num Out Delimiter=32
Analysis Text=Height=-16,FStyle=0,Color=12,Name=Arial
Analysis Grid Color=8
Analysis Graph Background=15
Object Default=Height=-16,FStyle=0,Color=4,Name=Arial
Analysis Window Background=15
NumOut=Height=-13,FStyle=0,Color=4,Name=Courier New
ScaleColor=On
Select Color=9
Select Box Color=4
Cursor Select Color Primary=7
Cursor Select Color Secondary=9
Tracker Intercept=False
Tracker Mouse=True
Tracker Cursor=True
Tracker Foreground=Height=-19,FStyle=0,Color=0,Name=Arial
Tracker Background=11
Data Point Labels Color Fore=Height=-19,FStyle=0,Color=0,Name=Arial
Data Point Labels Color Back=11
AnimateWait=0
AnimateWaitTime=500
Same Y Scales=Yes
T.Save_For_Future=No
A.Save_For_Future=No
D.Save_For_Future=No
T.Reduce_Display=1
T.Reduce_Save=1
A.Reduce_Display=1
A.Reduce_Save=1
D.Reduce_Display=1
D.Reduce_Save=1

[Tools]
Pos=Top
SELECT=Yes
GRAPHIC=No
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
POLYCLOS=No
SCALE=Yes
CURSOR=Yes
MEASUREH=Yes
MEASUREV=Yes
TAG=Yes
TEXT=Yes
PROPERTY=Yes
START=Yes
STOP=Yes
PAUSE=No
DATAPTS=Yes
TOKENS=Yes
RULER=No
PLUS=No
XAXIS=Yes
YAXIS=Yes
MINORLOG=No
BASELINE=No
HORIZCUR=No
GOTOX=Yes
GOTOY=Yes
GOTOPERF=Yes
GOTOBRNC=Yes
NEXT=Yes
NEXTIN=Yes
PEAK=Yes
VALLEY=Yes
HIGH=Yes
LOW=Yes
INFLECTN=Yes
GHIGH=Yes
GLOW=Yes
BOTTOM=Yes
TOP=Yes
AOUTPUT=Yes
ZOOMIN=No
ZOOMOUT=No
COLOR=Yes
FONT=Yes

[Monte Carlo Options]
Analysis=Transient
Status=Off
Distribution=Normal
Number of Runs

[Monte Carlo Options]
Analysis=AC
Status=Off
Distribution=Normal
Number of Runs

[Monte Carlo Options]
Analysis=DC
Status=Off
Distribution=Normal
Number of Runs

[Limits]
Analysis=Transient
OPT=120
Horizontal Cursor=False
Temperature Type=Linear

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
SFmtX=3
SFmtY=3
Line Color=12
Text Color=12

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
SFmtX=3
SFmtY=3
Line Color=9
Text Color=9

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
SFmtX=3
SFmtY=3
Line Color=2
Text Color=2

[Limits]
Analysis=AC
OPT=0
Horizontal Cursor=False
Temperature Type=Linear

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
SFmtX=3
SFmtY=3
Line Color=12
Text Color=12

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
SFmtX=3
SFmtY=3
Line Color=9
Text Color=9

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
SFmtX=3
SFmtY=3
Line Color=2
Text Color=2

[Limits]
Analysis=DC
OPT=0
Horizontal Cursor=False
Temperature Type=Linear
Sweep1 type=Auto
Sweep2 type=None

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
SFmtX=3
SFmtY=3
Line Color=12
Text Color=12

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
SFmtX=3
SFmtY=3
Line Color=9
Text Color=9

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
SFmtX=3
SFmtY=3
Line Color=2
Text Color=2

[Optimize]
Format=3

[Optimize]
Analysis=Transient
Method=Stepping_Powel

[Optimize]
Analysis=AC
Method=Stepping_Powel

[Optimize]
Analysis=DC
Method=Stepping_Powel

[Watch]
Format=3

[Watch]
Analysis=Transient
ExprPercentWidth=80

[Watch]
Analysis=AC
ExprPercentWidth=80

[Watch]
Analysis=DC
ExprPercentWidth=80

[DSP]
T.Status=Off
A.Status=Off

[TF]
Input Source
Place Text=False

[SENS]
Multiple=False
Parameter Type=Component
