[Main]
FileType=CIR
Version=7.00
Program=Micro-Cap
Screen=800,600
MCAPVersion=7.0.0.0
Key ID=493 834 421
NLCnt=15
TXCnt=16

[shapedef]
Name=Capacitor
Line=0,0,22,0
Line=22,-8,22,8
Line=26,-8,26,8
Line=26,0,48,0
Current=32,12,16,12

[shapedef]
Name=NFI
Root="Isource.Root",-12,0,0
Root="TextN.Root",-26,20,0
Root="TextF.Root",-18,20,0

[shapedef]
Name=TextF.Root
Line=0,0,5,0
Line=0,0,0,8
Line=2,4,0,4

[shapedef]
Name=Isource.Root
Ellipse=-12,12,12,36
Line=0,0,0,24
PolyClosed=3 ,Solid
PolyLine=-4,24
PolyLine=4,24
PolyLine=0,32
Line=0,32,0,48
Current=16,16,16,32

[shapedef]
Name=TextN.Root
Line=0,8,0,0
Line=0,0,5,8
Line=5,8,5,0

[compdef]
Name=NFI
Definition=NFI
Shape=NFI
Mask=4096
Label Offset=15,12,-29,13
PinCnt=2
Pin="Plus",0,0,7,12
Pin="Minus",0,6,7,3

[compdef]
Name=Capacitor
Definition=Capacitor
Shape=Capacitor
Mask=7681
Label Offset=19,8,12,12
PinCnt=2
Pin="Plus",6,0,-3,-5
Pin="Minus",0,0,-14,-5

[Circuit]
WinBackGround Color=15
Grid Text Color=Height=-16,FStyle=0,Color=1,Name=Arial
Object Default=Height=-16,FStyle=0,Color=11,Name=Arial
Component Color=12
Attribute Text=Height=-16,FStyle=0,Color=2,Name=Arial
Wire Color=2
Select Color=5
Pin Color=13
Select Box Color=0
Node Number=Height=-12,FStyle=0,Color=9,Name=Arial
Node Voltage Color=12
Current=Height=-13,FStyle=0,Color=12,Name=Arial
Power/Condition=Height=-13,FStyle=0,Color=9,Name=Arial
Digital Path Color=9
Title Block=Height=-19,FStyle=0,Color=0,Name=Arial
Digital 0 Color=0
Digital R Color=11
Digital F Color=11
Digital 1 Color=9
Digital X Color=7
Digital Z Color=8
Window Placement=2,3, -1,-1, -6,-25, 44,44,686,390
Window Placement in Analysis=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Block Select Color=41
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=Page $page of $maxpage
TitleBlock One Title=True
Title_Block_Border=False
Title_Block=False

[Wire]
Grids=39,26,46,26

[Comp]
Name=NFI
Grid=46,32
Rot=4

[Attr]
ONV=18,-30,PART,Tr
Style=8192
Height=-12
Color=9

[Attr]
ONV=-243,18,VALUE,-K*pow((V(PLATE)-(1+MU)*V(CATH)+MU*V(GRID)),1.5)
Style=8192
Color=9

[Comp]
Name=Capacitor
Grid=54,26
Rot=1

[Attr]
ONV=14,10,PART,C1
Style=8192
Height=-12
Color=9

[Attr]
ONV=11,28,VALUE,CPC
Style=8192
Height=-12
Color=9

[Comp]
Name=Capacitor
Grid=39,26
Rot=6

[Attr]
ONV=-33,-25,PART,C2
Style=8192
Height=-12
Color=9

[Attr]
ONV=-35,11,VALUE,CGP
Style=8192
Height=-12
Color=9

[Wire]
Grids=27,32,46,32

[Comp]
Name=Capacitor
Grid=27,26
Rot=1

[Attr]
ONV=11,10,PART,C3
Style=8192
Height=-12
Color=9

[Attr]
ONV=10,26,VALUE,CGC
Style=8192
Height=-12
Color=9

[Wire]
Grids=16,32,27,32

[Wire]
Grids=15,32,16,32

[Wire]
Grids=15,26,16,26

[Wire]
Grids=16,26,27,26

[Wire]
Grids=27,26,33,26

[Wire]
Grids=54,26,58,26

[Wire]
Grids=49,26,54,26

[Wire]
Grids=46,32,54,32

[Wire]
Grids=46,26,49,26

[Node Offsets]

[Condition Offsets]

[Grid Text]
Text=.HELP K "Tube constant k"
Grid=17,43

[Grid Text]
Text=Plate
Grid=49,26
Height=-12
Color=9

[Grid Text]
Text=Grid
Grid=16,26
Height=-12
Color=9

[Grid Text]
Text=Cath
Grid=16,32
Height=-12
Color=9

[Grid Text]
Text=The Triode macro is implemented with a 3/2 power function
Grid=10,13
Height=-12
Color=9

[Grid Text]
Text=.PARAMETERS (K=5M,MU=.05,CGP=10P,CGC=10P,CPC=10P)
Grid=17,40
Color=5

[Grid Text]
Text=source. The model uses a voltage-controlled current source.
Grid=10,15
Height=-12
Color=9

[Grid Text]
Text=The k, Mu, Cgp, Cgc, and Cpc values are passed as parameters
Grid=10,17
Height=-12
Color=9

[Grid Text]
Text=when the macro is used in a circuit.  For example, a typical
Grid=10,19
Height=-12
Color=9

[Grid Text]
Text=macro parameter call would be Triode(1E-5,20,1nf,2nf,.1nf).
Grid=10,21
Height=-12
Color=9

[Grid Text]
Text=TRIODE MACRO
Grid=27,6
Height=-19
Color=13

[Grid Text]
Text=Called by other circuits.  Not intended for stand alone analysis.
Grid=10,10
Height=-19
Color=9

[Grid Text]
Text=.HELP MU "Tube constant mu"
Grid=17,46

[Grid Text]
Text=.HELP CGP "Grid to plate capacitance "
Grid=17,49

[Grid Text]
Text=.HELP CGC "Grid to cathode capacitance"
Grid=17,52

[Grid Text]
Text=.HELP CPC "Plate to cathode capacitance"
Grid=17,55

[Schematic]
Page 0=0
TabSize 0=320
Page 1=0
TabSize 1=320
Page 2=0
TabSize 2=320
Page 3=0
TabSize 3=320
Splitter.xs=0
Splitter.ys=0
TextQuad=4099
Scale=0.6666666666666666
PrinterScale=1
View=304

[Tools]
Pos=Top
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
FLAG=No
META=No
INFO=Yes
HELP=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=No
GRID=Yes
BORDER=No
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FILPX=Yes
FINDCOMP=No
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
TOFRONT=No
TOBACK=No
PAGEADD=No
PAGEDEL=No
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=No
COLOR=Yes
FONT=Yes

[Page]
Index=0
Name=Page 1
Scale 0=0.6666666666666666
Scale 1=1
Scale 2=1
Scale 3=1
Grid=70,53

[Text Area]
Font=Height=-12,FStyle=0,Color=9,Name=Courier New
Comment Color=8
Background Color=15
Len=0


[Printer]
T.AutoTile=No
T.BlackBorder=No
A.AutoTile=No
A.BlackBorder=No
D.AutoTile=No
D.BlackBorder=No

[TRANSIENT]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[AC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[DC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[Analysis]
Window Placement=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Num Out Header Left
Num Out Header Center=$MC\n$user\n$company\n$Analysis of $name\n
Num Out Header Right
Num Out Delimiter=32
Analysis Text=Height=-12,FStyle=0,Color=4,Name=Arial
Analysis Grid Color=7
Analysis Graph Background=7
Object Default=Height=-16,FStyle=0,Color=0,Name=Arial
Analysis Window Background=15
NumOut=Height=-12,FStyle=0,Color=9,Name=Courier New
ScaleColor=On
Select Color=9
Select Box Color=4
Cursor Select Color Primary=7
Cursor Select Color Secondary=9
Tracker Intercept=False
Tracker Mouse=True
Tracker Cursor=True
Tracker Foreground=Height=-19,FStyle=0,Color=0,Name=Arial
Tracker Background=11
Data Point Labels Color Fore=Height=-19,FStyle=0,Color=0,Name=Arial
Data Point Labels Color Back=11
AnimateWait=0
AnimateWaitTime=500
Same Y Scales=Yes
T.Save_For_Future=No
A.Save_For_Future=No
D.Save_For_Future=No
T.Reduce_Display=1
T.Reduce_Save=1
A.Reduce_Display=1
A.Reduce_Save=1
D.Reduce_Display=1
D.Reduce_Save=1

[Tools]
Pos=Top
SELECT=Yes
GRAPHIC=No
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
POLYCLOS=No
SCALE=Yes
CURSOR=Yes
MEASUREH=Yes
MEASUREV=Yes
TAG=Yes
TEXT=Yes
PROPERTY=Yes
START=Yes
STOP=Yes
PAUSE=No
DATAPTS=Yes
TOKENS=Yes
RULER=No
PLUS=No
XAXIS=Yes
YAXIS=Yes
MINORLOG=No
BASELINE=No
HORIZCUR=No
GOTOX=Yes
GOTOY=Yes
GOTOPERF=Yes
GOTOBRNC=Yes
NEXT=Yes
NEXTIN=Yes
PEAK=Yes
VALLEY=Yes
HIGH=Yes
LOW=Yes
INFLECTN=Yes
GHIGH=Yes
GLOW=Yes
BOTTOM=Yes
TOP=Yes
AOUTPUT=Yes
ZOOMIN=No
ZOOMOUT=No
COLOR=Yes
FONT=Yes

[Monte Carlo Options]
Analysis=Transient
Status=Off
Distribution=Normal
Number of Runs=1

[Monte Carlo Options]
Analysis=AC
Status=Off
Distribution=Normal
Number of Runs=1

[Monte Carlo Options]
Analysis=DC
Status=Off
Distribution=Normal
Number of Runs=1

[Limits]
Analysis=Transient
TRange=5ms
TStep=0.0001
NPts=50
Temp=27
OPT=88
Horizontal Cursor=False
Temperature Type=Linear

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
XExp=T
YExp=Plate
XRng=5ms
YRng=300,250
Range Grid X=0.001
Range Grid Y=10
VFmtX=3
SFmtX=2
SFmtY=2

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
XExp=T
YExp=Grid
XRng=5ms
YRng=-11,-9
Range Grid X=0.001
Range Grid Y=0.4
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=1
Text Color=1

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=2
Text Color=2

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=3
Text Color=3

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=4
Text Color=4

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=5
Text Color=5

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=6
Text Color=6

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=7
Text Color=7

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=8
Text Color=8

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=9
Text Color=9

[Limits]
Analysis=AC
FRange=1E8,1
NPts=50
Temp=27
MaxChng=5
NInput=grid
NOutput=Plate
OPT=88
Horizontal Cursor=False
Temperature Type=Linear

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
XExp=f
YExp=db(mag(v(Plate)/v(grid)))
XRng=1E8,1
YRng=40,-60
Range Grid Y=20
VFmtX=3
SFmtX=2
SFmtY=2

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=2
XExp=f
YExp=inoise
XRng=1E8,1
YRng=0,-400
Range Grid Y=80
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=1
Text Color=1

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
XExp=f
YExp=re(v(Plate)/v(grid))
XRng=1E8,1
YRng=1.0,-1.0
Range Grid Y=0.4
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=2
Text Color=2

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
XExp=f
YExp=im(v(Plate)/v(grid))
XRng=1E8,1
YRng=1.0,-1.0
Range Grid Y=0.4
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=3
Text Color=3

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=2
XExp=f
YExp=ph(v(Plate)/v(grid))
XRng=1E8,1
YRng=90,-360
Range Grid Y=90
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=4
Text Color=4

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=3
XExp=f
YExp=gd(v(Plate)/v(grid))
XRng=1E8,1
YRng=1E-4,1E-9
Range Grid Y=1.99998e-5
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=5
Text Color=5

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=6
Text Color=6

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=7
Text Color=7

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=8
Text Color=8

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=9
Text Color=9

[Limits]
Analysis=DC
I2Range=0,-18,2
I2=Grid
I1Range=500,0
I1=VEE
NPts=5
Temp=27
MaxChng=2
OPT=24
Horizontal Cursor=False
Temperature Type=Linear
Sweep1 type=Auto
Sweep2 type=Linear

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
XExp=VEE
YExp=VEE,PLate,I
XRng=500,0,5
YRng=50ma
Range Grid X=100
Range Grid Y=0.01
VFmtX=3
SFmtX=2
SFmtY=2

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=1
Text Color=1

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=2
Text Color=2

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=3
Text Color=3

[Stepping]
Analysis=Transient
Index=1
Parameter Type=Component
Param=Value

[Stepping]
Analysis=AC
Index=1
Parameter Type=Component
Param=Value

[Stepping]
Analysis=DC
Index=1
Parameter Type=Component
Param=Value

[Optimize]
Format=3

[Optimize]
Analysis=Transient
Method=Stepping_Powel

[Optimize]
Analysis=AC
Method=Stepping_Powel

[Optimize]
Analysis=DC
Method=Stepping_Powel

[Watch]
Format=3

[Watch]
Analysis=Transient
ExprPercentWidth=80

[Watch]
Analysis=AC
ExprPercentWidth=80

[Watch]
Analysis=DC
ExprPercentWidth=80

[DSP]
T.Status=Off
A.Status=Off

[TF]
Input Source
Place Text=False

[SENS]
Multiple=False
Parameter Type=Component
