[Main]
FileType=CIR
Version=7.00
Program=Micro-Cap
Screen=800,600
MCAPVersion=7.0.0.0
Key ID=493 834 421
NLCnt=16
TXCnt=13

[shapedef]
Name=Resistor
PolyOpen=12 
PolyLine=0,0
PolyLine=0,0
PolyLine=12,0
PolyLine=14,-4
PolyLine=18,4
PolyLine=22,-4
PolyLine=26,4
PolyLine=30,-4
PolyLine=34,4
PolyLine=36,0
PolyLine=48,0
PolyLine=48,0
Current=32,8,16,8

[shapedef]
Name=Capacitor
Line=0,0,22,0
Line=22,-8,22,8
Line=26,-8,26,8
Line=26,0,48,0
Current=32,12,16,12

[shapedef]
Name=NFV
Root="Vsource.root",0,-12,0
Root="TextNv.Root",20,-6,0
Root="TextFv.Root",20,1,0

[shapedef]
Name=IOFV
Root="IOFV.Root",-2,-2,0

[shapedef]
Name=Ground
Line=0,0,12,0
Line=12,-8,12,8
Line=18,-4,18,4
Line=24,0,24,0

[shapedef]
Name=Vsource.root
Line=0,0,12,0
Line=36,0,48,0
Ellipse=12,-12,36,12
Line=7,5,7,9
Root="Plus.root",39,5,0
Current=32,16,16,16

[shapedef]
Name=Plus.root
Line=-2,0,2,0
Line=0,-2,0,2

[shapedef]
Name=OFV.Root
Root="Plus.root",6,6,0
Ellipse=-2,-2,2,2
Ellipse=-2,46,2,50

[shapedef]
Name=TextNv.Root
Line=0,0,8,0
Line=8,0,0,5
Line=0,5,8,5

[shapedef]
Name=TextFv.Root
Line=0,0,8,0
Line=4,0,4,2
Line=8,0,8,5

[shapedef]
Name=Isource.Root
Ellipse=-12,12,12,36
Line=0,0,0,24
PolyClosed=3 ,Solid
PolyLine=-4,24
PolyLine=4,24
PolyLine=0,32
Line=0,32,0,48
Current=16,16,16,32

[shapedef]
Name=IOFV.Root
Root="Isource.Root",36,0,0
Root="OFV.Root",-2,-2,0
Current=64,16,64,32

[compdef]
Name=Ground
Definition=Ground
Shape=Ground
Mask=4865
Label Offset=0,0,0,0
PinCnt=1
Pin="PinA",0,0,-3,-7

[compdef]
Name=NFV
Definition=NFV
Shape=NFV
Mask=4864
Label Offset=18,12,16,13
PinCnt=2
Pin="Plus",6,0,-8,-4
Pin="Minus",0,0,-21,-6

[compdef]
Name=IofV
Definition=IofV
Shape=IOFV
Mask=4096
Label Offset=63,11,-31,60
PinCnt=4
Pin="Plus Output",6,0,-18,-3
Pin="Minus Output",6,6,-12,17
Pin="Plus Input",0,0,-36,-4
Pin="Minus Input",0,6,-32,17

[compdef]
Name=Capacitor
Definition=Capacitor
Shape=Capacitor
Mask=7681
Label Offset=19,8,12,12
PinCnt=2
Pin="Plus",6,0,-3,-5
Pin="Minus",0,0,-14,-5

[compdef]
Name=Resistor
Definition=Resistor
Shape=Resistor
Mask=7681
Label Offset=18,6,8,11
PinCnt=2
Pin="Plus",6,0,-10,-4
Pin="Minus",0,0,-14,-4

[Circuit]
WinBackGround Color=15
Grid Text Color=Height=-16,FStyle=0,Color=1,Name=Arial
Object Default=Height=-16,FStyle=0,Color=11,Name=Arial
Component Color=3
Attribute Text=Height=-16,FStyle=0,Color=2,Name=Arial
Wire Color=0
Select Color=0
Pin Color=0
Select Box Color=0
Node Number=Height=-12,FStyle=0,Color=1,Name=Arial
Node Voltage Color=12
Current=Height=-13,FStyle=0,Color=12,Name=Arial
Power/Condition=Height=-13,FStyle=0,Color=9,Name=Arial
Digital Path Color=9
Title Block=Height=-19,FStyle=0,Color=0,Name=Arial
Digital 0 Color=0
Digital R Color=11
Digital F Color=11
Digital 1 Color=9
Digital X Color=7
Digital Z Color=8
Window Placement=2,3, -1,-1, -6,-25, 66,66,708,412
Window Placement in Analysis=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Block Select Color=41
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=Page $page of $maxpage
TitleBlock One Title=True
Title_Block_Border=False
Title_Block=False

[Wire]
Grids=55,31,61,31

[Wire]
Grids=54,31,55,31

[Comp]
Name=Ground
Grid=37,37
Rot=7

[Comp]
Name=NFV
Grid=54,37
Rot=3

[Attr]
ONV=21,-30,PART,VCO
Style=8192
Height=-12
Color=0

[Attr]
ONV=-115,7,VALUE,VP*COS(2*PI*(F0*T+KF*v(VMOD)))
Style=8192
Height=-12
Color=0

[Comp]
Name=IofV
Grid=22,31

[Attr]
ONV=63,18,PART,G
Style=8192
Height=-12
Color=0

[Attr]
ONV=20,17,VALUE,-1
Style=8192
Height=-12
Color=0

[Wire]
Grids=18,37,22,37

[Wire]
Grids=28,37,37,37

[Comp]
Name=Capacitor
Grid=45,37
Rot=3

[Attr]
ONV=14,-42,PART,C1
Style=8192
Height=-12
Color=0

[Attr]
ONV=17,-28,VALUE,1 IC=0
Style=8192
Height=-12
Color=0

[Wire]
Grids=28,31,34,31

[Comp]
Name=Resistor
Grid=37,31
Rot=1

[Attr]
ONV=11,8,PART,R2
Style=8192
Height=-12
Color=0

[Attr]
ONV=9,27,VALUE,1E6
Style=8192
Height=-12
Color=0

[Wire]
Grids=37,37,45,37

[Wire]
Grids=37,31,45,31

[Wire]
Grids=22,37,28,37

[Wire]
Grids=45,37,54,37

[Wire]
Grids=14,31,22,31

[Wire]
Grids=34,31,37,31

[Node Offsets]

[Condition Offsets]

[Grid Text]
Text=.HELP VP "Peak magnitude of the output signal"
Grid=18,49

[Grid Text]
Text=VMOD
Grid=34,31
Height=-12
Color=0

[Grid Text]
Text=PINB
Grid=55,31
Height=-12
Color=0

[Grid Text]
Text=PINA
Grid=14,31
Height=-12
Color=0

[Grid Text]
Text=.PARAMETERS(VP=1,F0=1Meg,KF=.1Meg)
Grid=17,44
Height=-12
Color=0

[Grid Text]
Text=INPUT PARAMETERS ARE:
Grid=16,22
Height=-12
Color=0

[Grid Text]
Text=VP...THE PEAK MAGNITUDE OF THE OUTPUT SIGNAL
Grid=16,24
Height=-12
Color=0

[Grid Text]
Text=F0...THE CENTER FREQUENCY
Grid=16,26
Height=-12
Color=0

[Grid Text]
Text=KF...THE FREQUENCY SENSITIVITY IN HZ/VOLT
Grid=16,28
Height=-12
Color=0

[Grid Text]
Text=VCO MACRO
Grid=23,13
Height=-19
Color=13

[Grid Text]
Text=Called by other circuits.  Not intended for stand alone analysis.
Grid=3,17
Height=-19
Color=9

[Grid Text]
Text=.HELP F0 "Center frequency"
Grid=18,51

[Grid Text]
Text=.HELP KF "Frequency sensitivity in Hz/Volt"
Grid=18,53

[Schematic]
Page 0=0
TabSize 0=320
Page 1=0
TabSize 1=320
Page 2=0
TabSize 2=320
Page 3=0
TabSize 3=320
Splitter.xs=0
Splitter.ys=0
TextQuad=1
Scale=1
PrinterScale=1
View=304

[Tools]
Pos=Top
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
FLAG=No
META=No
INFO=Yes
HELP=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=No
GRID=Yes
BORDER=No
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FILPX=Yes
FINDCOMP=No
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
TOFRONT=No
TOBACK=No
PAGEADD=No
PAGEDEL=No
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=No
COLOR=Yes
FONT=Yes

[Page]
Index=0
Name=Page 1
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=64,57

[Text Area]
Font=Height=-12,FStyle=0,Color=0,Name=Courier New
Comment Color=8
Background Color=15
Len=0


[Printer]
T.AutoTile=No
T.BlackBorder=No
A.AutoTile=No
A.BlackBorder=No
D.AutoTile=No
D.BlackBorder=No

[TRANSIENT]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[AC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[DC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[Analysis]
Window Placement=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Num Out Header Left
Num Out Header Center=$MC\n$user\n$company\n$Analysis of $name\n
Num Out Header Right
Num Out Delimiter=32
Analysis Text=Height=-12,FStyle=0,Color=10,Name=Arial
Analysis Grid Color=7
Analysis Graph Background=7
Object Default=Height=-16,FStyle=0,Color=0,Name=Arial
Analysis Window Background=15
NumOut=Height=-12,FStyle=0,Color=9,Name=Courier New
ScaleColor=On
Select Color=9
Select Box Color=4
Cursor Select Color Primary=7
Cursor Select Color Secondary=9
Tracker Intercept=False
Tracker Mouse=True
Tracker Cursor=True
Tracker Foreground=Height=-19,FStyle=0,Color=0,Name=Arial
Tracker Background=11
Data Point Labels Color Fore=Height=-19,FStyle=0,Color=0,Name=Arial
Data Point Labels Color Back=11
AnimateWait=0
AnimateWaitTime=500
Same Y Scales=Yes
T.Save_For_Future=No
A.Save_For_Future=No
D.Save_For_Future=No
T.Reduce_Display=1
T.Reduce_Save=1
A.Reduce_Display=1
A.Reduce_Save=1
D.Reduce_Display=1
D.Reduce_Save=1

[Tools]
Pos=Top
SELECT=Yes
GRAPHIC=No
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
POLYCLOS=No
SCALE=Yes
CURSOR=Yes
MEASUREH=Yes
MEASUREV=Yes
TAG=Yes
TEXT=Yes
PROPERTY=Yes
START=Yes
STOP=Yes
PAUSE=No
DATAPTS=Yes
TOKENS=Yes
RULER=No
PLUS=No
XAXIS=Yes
YAXIS=Yes
MINORLOG=No
BASELINE=No
HORIZCUR=No
GOTOX=Yes
GOTOY=Yes
GOTOPERF=Yes
GOTOBRNC=Yes
NEXT=Yes
NEXTIN=Yes
PEAK=Yes
VALLEY=Yes
HIGH=Yes
LOW=Yes
INFLECTN=Yes
GHIGH=Yes
GLOW=Yes
BOTTOM=Yes
TOP=Yes
AOUTPUT=Yes
ZOOMIN=No
ZOOMOUT=No
COLOR=Yes
FONT=Yes

[Monte Carlo Options]
Analysis=Transient
Status=Off
Distribution=Normal
Number of Runs=1

[Monte Carlo Options]
Analysis=AC
Status=Off
Distribution=Normal
Number of Runs

[Monte Carlo Options]
Analysis=DC
Status=Off
Distribution=Normal
Number of Runs

[Limits]
Analysis=Transient
TRange=50
TStep=1
NPts=5000
Temp=27
OPT=24
Horizontal Cursor=False
Temperature Type=Linear

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
XExp=T
YExp=Vco
XRng=50,40
YRng=1,-1
Range Grid X=2
Range Grid Y=0.4
VFmtX=3
SFmtX=2
SFmtY=2

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
XExp=T
YExp=Vco
XRng=50,40
YRng=1,-1
Range Grid X=2
Range Grid Y=0.4
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=1
Text Color=1

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=2
XExp=T
YExp=Ramp
XRng=50,40
YRng=1
Range Grid X=2
Range Grid Y=0.2
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=2
Text Color=2

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
Plt=2
XExp=T
YExp=Vmod
XRng=50,40
YRng=5
Range Grid X=2
Range Grid Y=1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=3
Text Color=3

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=4
Text Color=4

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=5
Text Color=5

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=6
Text Color=6

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=7
Text Color=7

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=8
Text Color=8

[WaveForm]
Analysis=Transient
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=9
Text Color=9

[Limits]
Analysis=AC
NPts=50
OPT=64
Horizontal Cursor=False
Temperature Type=Linear

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
XExp=f
YExp=db(mag(v()/v()))
VFmtX=3
SFmtX=2
SFmtY=2

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=2
XExp=f
YExp=inoise
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=1
Text Color=1

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
XExp=f
YExp=re(v()/v())
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=2
Text Color=2

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=1
XExp=f
YExp=im(v()/v())
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=3
Text Color=3

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=2
XExp=f
YExp=ph(v()/v())
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=4
Text Color=4

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
Plt=3
XExp=f
YExp=gd(v()/v())
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=5
Text Color=5

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=6
Text Color=6

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=7
Text Color=7

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=8
Text Color=8

[WaveForm]
Analysis=AC
Options=LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=9
Text Color=9

[Limits]
Analysis=DC
NPts=0
OPT=0
Horizontal Cursor=False
Temperature Type=Linear
Sweep1 type=Auto
Sweep2 type=None

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
Plt=1
VFmtX=3
SFmtX=2
SFmtY=2

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=1
Text Color=1

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=2
Text Color=2

[WaveForm]
Analysis=DC
Options=LINEARX,LINEARY
AliasID=-1
VFmtX=3
SFmtX=2
SFmtY=2
Line Color=3
Text Color=3

[Optimize]
Format=3

[Optimize]
Analysis=Transient
Method=Stepping_Powel

[Optimize]
Analysis=AC
Method=Stepping_Powel

[Optimize]
Analysis=DC
Method=Stepping_Powel

[Watch]
Format=3

[Watch]
Analysis=Transient
ExprPercentWidth=80

[Watch]
Analysis=AC
ExprPercentWidth=80

[Watch]
Analysis=DC
ExprPercentWidth=80

[DSP]
T.Status=Off
A.Status=Off

[TF]
Input Source
Place Text=False

[SENS]
Multiple=False
Parameter Type=Component
