[Main]
FileType=CIR
Version=8.01
Program=Micro-Cap
Screen=1600,1200
MCAPVersion=1.2.3.4
Key ID=123 456 789
NLCnt=130
TXCnt=27

[shapedef]
Name=Battery
Line=0,0,22,0
Line=22,-3,22,3
Line=26,-7,26,7
Line=26,0,48,0
Current=32,8,16,8

[shapedef]
Name=Resistor
PolyOpen=12 
PolyLine=0,0
PolyLine=0,0
PolyLine=12,0
PolyLine=14,-4
PolyLine=18,4
PolyLine=22,-4
PolyLine=26,4
PolyLine=30,-4
PolyLine=34,4
PolyLine=36,0
PolyLine=48,0
PolyLine=48,0
Current=32,8,16,8

[shapedef]
Name=Capacitor
Line=0,0,22,0
Line=22,-8,22,8
Line=26,-8,26,8
Line=26,0,48,0
Current=32,12,16,12

[shapedef]
Name=Opamp5
Root="Opamp.root",0,-4,0
Root="Plus.root",23,-6,0
Root="Minus.root",23,52,0
Line=32,56,32,34
Line=32,-8,32,13

[shapedef]
Name=Ground
Line=0,0,12,0
Line=12,-8,12,8
Line=18,-4,18,4
Line=24,0,24,0

[shapedef]
Name=Opamp.root
Line=0,48,6,48
Line=0,0,5,0
Line=6,-4,6,52
Line=6,-4,48,24
Line=6,52,48,24
Line=48,24,72,24
Line=10,12,14,12
Line=12,10,12,14
Line=10,36,14,36
Line=4,0,6,0

[shapedef]
Name=Minus.root
Line=-2,0,2,0

[shapedef]
Name=Plus.root
Line=-2,0,2,0
Line=0,-2,0,2

[compdef]
Name=C6_1%
Definition=Resistor
Shape=Resistor
Mask=6272
Label Offset=18,8,9,12
PinCnt=2
Pin="Plus",6,0,-8,-2
Pin="Minus",0,0,-14,-2

[compdef]
Name=LF147
Definition=Opamp
Shape=Opamp5
Mask=4224
memo=Wide bandwidth quad JFET i/p opamp
Label Offset=51,32,-15,46
PinCnt=5
Pin="Plus input",0,0,-30,-3
Pin="Minus input",0,6,-36,17
Pin="VEE",4,7,6,5
Pin="Output",9,3,-13,-4
Pin="VCC",4,-1,6,4

[compdef]
Name=Capacitor
Definition=Capacitor
Shape=Capacitor
Mask=7681
memo=Capacitor
Label Offset=19,8,12,12
PinCnt=2
Pin="Plus",6,0,-3,-5
Pin="Minus",0,0,-14,-5

[compdef]
Name=Ground
Definition=Ground
Shape=Ground
Mask=1793
memo=Ground
Label Offset=0,0,0,0
PinCnt=1
Pin="PinA",0,0,-3,-7

[compdef]
Name=Battery
Definition=Battery
Shape=Battery
Mask=5889
memo=Battery
Label Offset=19,7,10,13
PinCnt=2
Pin="Plus",6,0,-4,-5
Pin="Minus",0,0,-10,-5

[Circuit]
Window Placement=2,3, -1,-1, -4,-30, 220,290,1556,1014
Default Object=Color=4
Default Object Font=Height=-15,FStyle=0,Color=4,Name=Arial
Default Object Apply Border To Text=No
Default Object Apply Fill To Text=No
WinBackGround Color=15
Select Color=9
Select Box Color=4
Grid Text Color=Height=-12,FStyle=0,Color=1,Name=Arial
Component Color=12
Attribute Text=Height=-12,FStyle=0,Color=2,Name=Arial
Wire Color=2
Pin Connection=Height=-10,FStyle=0,Color=9,Name=Arial
Node Number=Height=-11,FStyle=0,Color=13,Name=Arial
Node Voltage Color=0
Dynamic AC Voltage Color=56
Text Banner Text=Height=-15,FStyle=0,Color=1,Name=Arial
Title Block Background=7
Current=Height=-11,FStyle=0,Color=12,Name=Arial
Power/Condition=Height=-11,FStyle=0,Color=9,Name=Arial
Digital Path Color=9
Title Block=Height=-15,FStyle=0,Color=0,Name=Arial
Digital 0 Color=0
Digital R Color=11
Digital F Color=11
Digital 1 Color=9
Digital X Color=7
Digital Z Color=8
SpiceType=AMBIGUOUS
Block Select Color=41
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=Page $page of $maxpage
TitleBlock One Title=False
Title_Block_Border=False
Title_Block=False

[Comp]
Name=C6_1%
Grid=49,17
Rot=4

[Attr]
ONV=18,-21,PART,R1
Style=8192

[Attr]
ONV=-1,11,VALUE,41.54778K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=50,31
Rot=5

[Attr]
ONV=13,-42,PART,R2
Style=8192

[Attr]
ONV=7,-24,VALUE,2.43867MEG
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=61,24

[Attr]
ONV=18,18,PART,X1
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=36,24
Rot=2

[Attr]
ONV=-35,-23,PART,C1
Style=8192

[Attr]
ONV=-38,11,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=47,24
Rot=2

[Attr]
ONV=-35,-23,PART,C2
Style=8192

[Attr]
ONV=-42,14,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=70,27,70,34

[Wire]
Grids=36,24,38,24

[Wire]
Grids=50,24,61,24

[Wire]
Grids=38,17,38,24

[Wire]
Grids=38,17,49,17

[Wire]
Grids=55,17,70,17

[Wire]
Grids=70,17,70,24

[Wire]
Grids=61,34,70,34

[Wire]
Grids=61,30,61,34

[Comp]
Name=Ground
Grid=50,34
Rot=7

[Wire]
Grids=50,31,50,34

[Wire]
Grids=50,24,50,25

[Wire]
Grids=70,24,70,27

[Wire]
Grids=47,24,50,24

[Wire]
Grids=38,24,41,24

[Wire]
Grids=27,24,30,24

[Comp]
Name=C6_1%
Grid=92,17
Rot=4

[Attr]
ONV=18,-21,PART,R5
Style=8192

[Attr]
ONV=-1,11,VALUE,121.81192K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=93,31
Rot=5

[Attr]
ONV=13,-42,PART,R6
Style=8192

[Attr]
ONV=7,-24,VALUE,831.78382K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=104,24

[Attr]
ONV=18,18,PART,X2
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=79,24
Rot=2

[Attr]
ONV=-35,-23,PART,C3
Style=8192

[Attr]
ONV=-38,11,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=90,24
Rot=2

[Attr]
ONV=-35,-23,PART,C4
Style=8192

[Attr]
ONV=-42,14,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=113,27,113,34

[Wire]
Grids=79,24,81,24

[Wire]
Grids=93,24,104,24

[Wire]
Grids=81,17,81,24

[Wire]
Grids=81,17,92,17

[Wire]
Grids=98,17,113,17

[Wire]
Grids=113,17,113,24

[Wire]
Grids=104,34,113,34

[Wire]
Grids=104,30,104,34

[Comp]
Name=Ground
Grid=93,34
Rot=7

[Wire]
Grids=93,31,93,34

[Wire]
Grids=93,24,93,25

[Wire]
Grids=113,24,113,27

[Wire]
Grids=90,24,93,24

[Wire]
Grids=81,24,84,24

[Wire]
Grids=70,24,73,24

[Comp]
Name=C6_1%
Grid=135,17
Rot=4

[Attr]
ONV=18,-21,PART,R9
Style=8192

[Attr]
ONV=-1,11,VALUE,193.77478K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=136,31
Rot=5

[Attr]
ONV=13,-42,PART,R10
Style=8192

[Attr]
ONV=7,-24,VALUE,522.88117K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=147,24

[Attr]
ONV=18,18,PART,X3
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=122,24
Rot=2

[Attr]
ONV=-35,-23,PART,C5
Style=8192

[Attr]
ONV=-38,11,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=133,24
Rot=2

[Attr]
ONV=-35,-23,PART,C6
Style=8192

[Attr]
ONV=-42,14,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=156,27,156,34

[Wire]
Grids=122,24,124,24

[Wire]
Grids=136,24,147,24

[Wire]
Grids=124,17,124,24

[Wire]
Grids=124,17,135,17

[Wire]
Grids=141,17,156,17

[Wire]
Grids=156,17,156,24

[Wire]
Grids=147,34,156,34

[Wire]
Grids=147,30,147,34

[Comp]
Name=Ground
Grid=136,34
Rot=7

[Wire]
Grids=136,31,136,34

[Wire]
Grids=136,24,136,25

[Wire]
Grids=156,24,156,27

[Wire]
Grids=133,24,136,24

[Wire]
Grids=124,24,127,24

[Wire]
Grids=113,24,116,24

[Comp]
Name=C6_1%
Grid=178,17
Rot=4

[Attr]
ONV=18,-21,PART,R13
Style=8192

[Attr]
ONV=-1,11,VALUE,252.53221K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=179,31
Rot=5

[Attr]
ONV=13,-42,PART,R14
Style=8192

[Attr]
ONV=7,-24,VALUE,401.22083K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=190,24

[Attr]
ONV=18,18,PART,X4
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=165,24
Rot=2

[Attr]
ONV=-35,-23,PART,C7
Style=8192

[Attr]
ONV=-38,11,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=176,24
Rot=2

[Attr]
ONV=-35,-23,PART,C8
Style=8192

[Attr]
ONV=-42,14,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=199,27,199,34

[Wire]
Grids=165,24,167,24

[Wire]
Grids=179,24,190,24

[Wire]
Grids=167,17,167,24

[Wire]
Grids=167,17,178,17

[Wire]
Grids=184,17,199,17

[Wire]
Grids=199,17,199,24

[Wire]
Grids=190,34,199,34

[Wire]
Grids=190,30,190,34

[Comp]
Name=Ground
Grid=179,34
Rot=7

[Wire]
Grids=179,31,179,34

[Wire]
Grids=179,24,179,25

[Wire]
Grids=199,24,199,27

[Wire]
Grids=176,24,179,24

[Wire]
Grids=167,24,170,24

[Wire]
Grids=156,24,159,24

[Comp]
Name=C6_1%
Grid=221,17
Rot=4

[Attr]
ONV=18,-21,PART,R17
Style=8192

[Attr]
ONV=-1,11,VALUE,294.07999K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=222,31
Rot=5

[Attr]
ONV=13,-42,PART,R18
Style=8192

[Attr]
ONV=7,-24,VALUE,344.53614K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=233,24

[Attr]
ONV=18,18,PART,X5
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=208,24
Rot=2

[Attr]
ONV=-35,-23,PART,C9
Style=8192

[Attr]
ONV=-38,11,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=219,24
Rot=2

[Attr]
ONV=-35,-23,PART,C10
Style=8192

[Attr]
ONV=-42,14,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=242,27,242,34

[Wire]
Grids=208,24,210,24

[Wire]
Grids=222,24,233,24

[Wire]
Grids=210,17,210,24

[Wire]
Grids=210,17,221,17

[Wire]
Grids=227,17,242,17

[Wire]
Grids=242,17,242,24

[Wire]
Grids=233,34,242,34

[Wire]
Grids=233,30,233,34

[Comp]
Name=Ground
Grid=222,34
Rot=7

[Wire]
Grids=222,31,222,34

[Wire]
Grids=222,24,222,25

[Wire]
Grids=242,24,242,27

[Wire]
Grids=219,24,222,24

[Wire]
Grids=210,24,213,24

[Wire]
Grids=199,24,202,24

[Comp]
Name=C6_1%
Grid=264,17
Rot=4

[Attr]
ONV=18,-21,PART,R21
Style=8192

[Attr]
ONV=-1,11,VALUE,315.5867K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=265,31
Rot=5

[Attr]
ONV=13,-42,PART,R22
Style=8192

[Attr]
ONV=7,-24,VALUE,321.05657K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=276,24

[Attr]
ONV=18,18,PART,X6
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=251,24
Rot=2

[Attr]
ONV=-35,-23,PART,C11
Style=8192

[Attr]
ONV=-38,11,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=262,24
Rot=2

[Attr]
ONV=-35,-23,PART,C12
Style=8192

[Attr]
ONV=-42,14,VALUE,25p
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=285,27,285,34

[Wire]
Grids=251,24,253,24

[Wire]
Grids=265,24,276,24

[Wire]
Grids=253,17,253,24

[Wire]
Grids=253,17,264,17

[Wire]
Grids=270,17,285,17

[Wire]
Grids=285,17,285,24

[Wire]
Grids=276,34,285,34

[Wire]
Grids=276,30,276,34

[Comp]
Name=Ground
Grid=265,34
Rot=7

[Wire]
Grids=265,31,265,34

[Wire]
Grids=265,24,265,25

[Wire]
Grids=285,24,285,27

[Wire]
Grids=262,24,265,24

[Wire]
Grids=253,24,256,24

[Wire]
Grids=242,24,245,24

[Comp]
Name=Battery
Grid=6,11
Rot=3

[Attr]
ONV=-24,-28,PART,V3
Style=8192

[Attr]
ONV=-24,-43,VALUE,15
Style=8192

[Comp]
Name=Ground
Grid=6,11
Rot=7

[Comp]
Name=Battery
Grid=14,5
Rot=7

[Attr]
ONV=-24,13,PART,V4
Style=8192

[Attr]
ONV=-24,28,VALUE,15
Style=8192

[Comp]
Name=Ground
Grid=14,11
Rot=7

[Grid Text]
Text="VM"
Grid=65,31
CBorder=NONE

[Grid Text]
Text="VP"
Grid=65,23
CBorder=NONE

[Grid Text]
Text="Stage 1:Sallen-KeyþF1 = 1*U*U/(U*U+0.26105*U+1)þPoles = -0.13053, -0.99144jþPoles = -0.13053, -0.99144j"
Grid=37,44
CBorder=NONE

[Grid Text]
Text="VM"
Grid=108,31
CBorder=NONE

[Grid Text]
Text="VP"
Grid=108,23
CBorder=NONE

[Grid Text]
Text="Stage 2:Sallen-KeyþF2 = 1*U*U/(U*U+0.76537*U+1)þPoles = -0.38268, -0.92388jþPoles = -0.38268, -0.92388j"
Grid=80,44
CBorder=NONE

[Grid Text]
Text="VM"
Grid=151,31
CBorder=NONE

[Grid Text]
Text="VP"
Grid=151,23
CBorder=NONE

[Grid Text]
Text="Stage 3:Sallen-KeyþF3 = 1*U*U/(U*U+1.2175*U+1)þPoles = -0.60876, -0.79335jþPoles = -0.60876, -0.79335j"
Grid=124,44
CBorder=NONE

[Grid Text]
Text="VM"
Grid=194,31
CBorder=NONE

[Grid Text]
Text="VP"
Grid=194,23
CBorder=NONE

[Grid Text]
Text="Stage 4:Sallen-KeyþF4 = 1*U*U/(U*U+1.5867*U+1)þPoles = -0.79335, -0.60876jþPoles = -0.79335, -0.60876j"
Grid=167,44
CBorder=NONE

[Grid Text]
Text="VM"
Grid=237,31
CBorder=NONE

[Grid Text]
Text="VP"
Grid=237,23
CBorder=NONE

[Grid Text]
Text="Stage 5:Sallen-KeyþF5 = 1*U*U/(U*U+1.8478*U+1)þPoles = -0.92388, -0.38268jþPoles = -0.92388, -0.38268j"
Grid=210,44
CBorder=NONE

[Grid Text]
Text="VM"
Grid=280,31
CBorder=NONE

[Grid Text]
Text="VP"
Grid=280,23
CBorder=NONE

[Grid Text]
Text="Stage 6:Sallen-KeyþF6 = 1*U*U/(U*U+1.9829*U+1)þPoles = -0.99144, -0.13053jþPoles = -0.99144, -0.13053j"
Grid=253,44
CBorder=NONE

[Grid Text]
Text="VM"
Grid=14,5
CBorder=NONE

[Grid Text]
Text="VP"
Grid=6,5
CBorder=NONE

[Grid Text]
Text="Out"
Grid=285,24
CBorder=NONE

[Grid Text]
Text="In"
Grid=27,24
CBorder=NONE

[Grid Text]
Text="High-Pass Butterworth Sallen-KeyþGain=0dB Cutoff Frequency=20000Hz Ripple=1dB Order=12þImpedance Scale Factor=1, and OPAMP model=$IDEAL"
Grid=20,6
Color=12
CFill=7
CBorder=0

[Grid Text]
Text="LP = Ideal low-pass response based upon choice of filter type and response. þHP = Ideal high-pass response transformed from the low pass response.  þThe circuit above is designed to match this transfer response. "
Grid=27,53
CBorder=NONE

[Grid Text]
Text=".define U (S/(2*PI*20000))"
Grid=27,56
CBorder=NONE

[Grid Text]
Text=".define LP þ1/(U*U+0.26105*U+1)*þ1/(U*U+0.76537*U+1)*þ1/(U*U+1.2175*U+1)*þ1/(U*U+1.5867*U+1)*þ1/(U*U+1.8478*U+1)*þ1/(U*U+1.9829*U+1)*þ1"
Grid=27,73
CBorder=NONE

[Grid Text]
Text=".define HP þ1*U*U/(U*U+0.26105*U+1)*þ1*U*U/(U*U+0.76537*U+1)*þ1*U*U/(U*U+1.2175*U+1)*þ1*U*U/(U*U+1.5867*U+1)*þ1*U*U/(U*U+1.8478*U+1)*þ1*U*U/(U*U+1.9829*U+1)"
Grid=27,88
CBorder=NONE

[Schematic]
Page 0=0
TabSize 0=340
Page 1=0
TabSize 1=340
Page 2=0
TabSize 2=340
Page 3=0
TabSize 3=340
Splitter.xs=0
Splitter.ys=0
TextQuad=4099
Scale=1
PrinterScale=1
View=304
GridUser=10

[Tools]
Pos=Top
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
LEFTBRK=No
RIGHTBRK=No
BOTHBRK=No
FLAG=Yes
META=No
INFO=Yes
HELP=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=Yes
GRID=Yes
BORDER=Yes
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FILPX=Yes
FINDCOMP=Yes
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
TOFRONT=Yes
TOBACK=Yes
PAGEADD=Yes
PAGEDEL=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=Yes
COLOR=Yes
FONT=Yes

[Page]
Index=0
Print=True
Name=Main
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=1
Type=Text
Print=False
Name=Text
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=2
Type=Text
Print=False
Name=Models
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=3
Type=Info
Print=False
Name=Info
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Text Area]
Page=1
Font=Height=-15,FStyle=0,Color=4,Name=Courier New
Comment Color=8
Background Color=15
Len=0


[Text Area]
Page=2
Font=Height=-15,FStyle=0,Color=4,Name=Courier New
Comment Color=8
Background Color=15
Len=114
.MODEL $IDEAL OPA (Level=1 A=1E8 RoutAC=.5m RoutDC=1m)
.MODEL RM1 RES (R=1 LOT=1%)
.MODEL CM1 CAP (C=1 LOT=1%)


[Limits]
Analysis=DynamicAC
FirstValueDisplay=Mag
SecondValueDisplay=PhaseDeg
PlaceText=True

[Limits]
Analysis=DynamicDC
PlaceText=True

[Optimize]
Format=3
