[Main]
FileType=CIR
Version=7.00
Program=Micro-Cap
Screen=1280,1024
MCAPVersion=7.0.0.0
Key ID=12 345 678
NLCnt=107
TXCnt=36

[shapedef]
Name=Battery
Line=0,0,22,0
Line=22,-3,22,3
Line=26,-7,26,7
Line=26,0,48,0
Current=32,8,16,8

[shapedef]
Name=Resistor
PolyOpen=12 
PolyLine=0,0
PolyLine=0,0
PolyLine=12,0
PolyLine=14,-4
PolyLine=18,4
PolyLine=22,-4
PolyLine=26,4
PolyLine=30,-4
PolyLine=34,4
PolyLine=36,0
PolyLine=48,0
PolyLine=48,0
Current=32,8,16,8

[shapedef]
Name=Capacitor
Line=0,0,22,0
Line=22,-8,22,8
Line=26,-8,26,8
Line=26,0,48,0
Current=32,12,16,12

[shapedef]
Name=NFV
Root="Vsource.root",0,-12,0
Root="TextNv.Root",20,-6,0
Root="TextFv.Root",20,1,0

[shapedef]
Name=NFI
Root="Isource.Root",-12,0,0
Root="TextN.Root",-26,20,0
Root="TextF.Root",-18,20,0

[shapedef]
Name=Sum
Root="Circle.root",0,-12,0
Line=26,0,37,0
Line=32,-5,32,5

[shapedef]
Name=Nor2
Root="Nor.root",0,-18,0

[shapedef]
Name=Inv
Root="Inv.root",0,-16,0

[shapedef]
Name=Ground
Line=0,0,12,0
Line=12,-8,12,8
Line=18,-4,18,4
Line=24,0,24,0

[shapedef]
Name=Inv.root
Line=8,-16,8,16
Line=8,-16,40,0
Line=8,16,40,0
Line=0,0,8,0
Ellipse=40,-2,44,2
Line=44,0,47,0
Line=46,0,48,0

[shapedef]
Name=Circle.root
Ellipse=20,-12,44,12
Line=0,0,19,0
Line=32,32,32,12
Line=64,0,44,0
PolyClosed=3 ,Solid
PolyLine=13,-3
PolyLine=18,0
PolyLine=13,3
PolyClosed=3 ,Solid
PolyLine=32,14
PolyLine=35,19
PolyLine=29,19
Line=18,0,20,0

[shapedef]
Name=Vsource.root
Line=0,0,12,0
Line=36,0,48,0
Ellipse=12,-12,36,12
Line=7,5,7,9
Root="Plus.root",39,5,0
Current=32,16,16,16

[shapedef]
Name=Plus.root
Line=-2,0,2,0
Line=0,-2,0,2

[shapedef]
Name=Nor.root
Arc=5,-18,43,20 , 24,20,42,8
Line=0,0,10,0
Line=0,16,10,16
Line=24,-4,6,-4
Line=6,20,24,20
Arc=5,-4,43,34 , 42,8,24,-4
Ellipse=42,6,46,10
Line=46,8,48,8
Arc=0,-4,12,20 , 6,20,6,-4

[shapedef]
Name=TextNv.Root
Line=0,0,8,0
Line=8,0,0,5
Line=0,5,8,5

[shapedef]
Name=TextF.Root
Line=0,0,5,0
Line=0,0,0,8
Line=2,4,0,4

[shapedef]
Name=TextFv.Root
Line=0,0,8,0
Line=4,0,4,2
Line=8,0,8,5

[shapedef]
Name=Isource.Root
Ellipse=-12,12,12,36
Line=0,0,0,24
PolyClosed=3 ,Solid
PolyLine=-4,24
PolyLine=4,24
PolyLine=0,32
Line=0,32,0,48
Current=16,16,16,32

[shapedef]
Name=TextN.Root
Line=0,8,0,0
Line=0,0,5,8
Line=5,8,5,0

[shapedef]
Name=Dlyline
Rectangle=-8,-8,40,8
Line=-8,0,-16,0
Line=40,0,48,0
Line=-6,0,2,0
PolyClosed=5 ,Solid
PolyLine=2,-2
PolyLine=2,-2
PolyLine=4,0
PolyLine=2,2
PolyLine=2,2
Line=36,0,28,0
PolyClosed=5 ,Solid
PolyLine=36,-2
PolyLine=36,-2
PolyLine=38,0
PolyLine=36,2
PolyLine=36,2
PolyClosed=5 
PolyLine=8,4
PolyLine=8,4
PolyLine=12,-2
PolyLine=16,4
PolyLine=14,4
Line=22,-4,22,4
Line=18,-4,26,-4

[compdef]
Name=Capacitor
Definition=Capacitor
Shape=Capacitor
Mask=6913
Label Offset=19,8,12,12
PinCnt=2
Pin="Plus",6,0,-3,-5
Pin="Minus",0,0,-14,-5

[compdef]
Name=Ground
Definition=Ground
Shape=Ground
Mask=1793
Label Offset=0,0,0,0
PinCnt=1
Pin="PinA",0,0,-3,-7

[compdef]
Name=NFI
Definition=NFI
Shape=NFI
Mask=4096
Label Offset=15,12,-29,13
PinCnt=2
Pin="Plus",0,0,7,12
Pin="Minus",0,6,7,3

[compdef]
Name=NFV
Definition=NFV
Shape=NFV
Mask=4864
Label Offset=18,12,16,13
PinCnt=2
Pin="Plus",6,0,-8,-4
Pin="Minus",0,0,-21,-6

[compdef]
Name=Resistor1
Definition=Resistor
Shape=Resistor
Mask=6913
Label Offset=18,6,8,11
PinCnt=2
Pin="Plus",6,0,-10,-4
Pin="Minus",0,0,-14,-4

[compdef]
Name=Nor2
Definition=NOR
Shape=Nor2
Mask=4096
Data1=2
Label Offset=16,4,8,10
PinCnt=3
Pin="In0",0,0,-9,-1
Pin="In1",0,2,-9,-1
Pin="Out",6,1,-7,-3

[compdef]
Name=Battery1
Definition=Battery
Shape=Battery
Mask=5888
Label Offset=0,0,0,0
PinCnt=2
Pin="Plus",6,0,-4,-1
Pin="Minus",0,0,-14,-1

[compdef]
Name=Inverter
Definition=INV
Shape=Inv
Mask=5123
Data1=1
Label Offset=12,-6,11,21
PinCnt=2
Pin="In",0,0,-4,-2
Pin="Out",6,0,-10,-2

[compdef]
Name=Sum
Definition=Macro
Shape=Sum
Mask=4096
Label Offset=45,5,15,21
PinCnt=3
Pin="PinA",a,0,0,-9,-3
Pin="PinB",a,4,4,8,4
Pin="PinC",a,8,0,-7,-3

[compdef]
Name=Delay
Definition=Macro
Shape=Dlyline
Mask=4096
Label Offset=11,9,12,2
PinCnt=2
Pin="In",a,-2,0,-4,-2
Pin="Out",a,6,0,-6,-1

[Circuit]
WinBackGround Color=15
Grid Text Color=Height=-12,FStyle=0,Color=1,Name=Arial
Object Default=Height=-15,FStyle=0,Color=4,Name=Arial
Component Color=12
Attribute Text=Height=-12,FStyle=0,Color=2,Name=Arial
Wire Color=2
Select Color=9
Pin Connection=Height=-13,FStyle=0,Color=9,Name=Arial
Select Box Color=4
Node Number=Height=-11,FStyle=0,Color=13,Name=Arial
Node Voltage Color=0
Current=Height=-11,FStyle=0,Color=12,Name=Arial
Power/Condition=Height=-11,FStyle=0,Color=9,Name=Arial
Digital Path Color=9
Title Block=Height=-15,FStyle=0,Color=0,Name=Arial
Digital 0 Color=0
Digital R Color=11
Digital F Color=11
Digital 1 Color=9
Digital X Color=7
Digital Z Color=8
Window Placement=2,3, -1,-1, -6,-25, 110,110,1100,724
Window Placement in Analysis=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Block Select Color=41
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=Page $page of $maxpage
TitleBlock One Title=True
Title_Block_Border=False
Title_Block=False

[Comp]
Name=Capacitor
Grid=31,25
Rot=1

[Attr]
ONV=11,12,PART,C1
Style=8192
Color=0

[Attr]
ONV=14,27,VALUE,1M
Style=8192
Color=0

[Attr]
ONV=0,32,MODEL,
Color=0

[Attr]
ONV=0,44,SLIDER_MIN,1M

[Attr]
ONV=0,55,SLIDER_MAX,1M

[Wire]
Grids=40,31,49,31

[Comp]
Name=Ground
Grid=31,31
Rot=7

[Wire]
Grids=31,25,40,25

[Wire]
Grids=19,25,25,25

[Wire]
Grids=19,31,31,31

[Wire]
Grids=49,25,56,25

[Comp]
Name=NFI
Grid=19,31
Rot=4

[Attr]
ONV=15,-27,PART,GSAW
Style=8192

[Attr]
ONV=-65,15,VALUE,IMAX*(V(INA,INB)>0)
Style=8192

[Attr]
ONV=0,44,DERIVATIVE,Default

[Comp]
Name=NFV
Grid=49,31
Rot=3

[Attr]
ONV=17,-37,PART,EX
Style=8192

[Attr]
ONV=-38,4,VALUE,V(A)*(V(INA,INB)>0)
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Wire]
Grids=31,31,40,31

[Wire]
Grids=7,25,15,25

[Comp]
Name=Ground
Grid=67,31
Rot=1

[Comp]
Name=Resistor1
Grid=68,25
Rot=4

[Attr]
ONV=18,-21,PART,R2
Style=8192

[Attr]
ONV=18,-36,VALUE,1K
Style=8192

[Attr]
ONV=18,-66,SLIDER_MAX,1000

[Wire]
Grids=74,25,76,25

[Comp]
Name=NFV
Grid=67,31
Rot=3

[Attr]
ONV=-31,-28,PART,E7
Style=8192

[Attr]
ONV=-54,29,VALUE,(V(SAW)>=1)*4
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Comp]
Name=Nor2
Grid=80,25

[Attr]
ONV=16,4,PART,U1
Style=8192

[Attr]
ONV=16,19,TIMING MODEL,DLY_TTL

[Attr]
ONV=16,34,I/O MODEL,IO_STD

[Attr]
ONV=16,49,MNTYMXDLY,0

[Attr]
ONV=16,64,IO_LEVEL,0

[Attr]
ONV=16,79,POWER NODE,$G_DPWR

[Attr]
ONV=16,94,GROUND NODE,$G_DGND

[Comp]
Name=Capacitor
Grid=92,26
Rot=2

[Attr]
ONV=-35,-23,PART,C2
Style=8192

[Attr]
ONV=-42,17,VALUE,CDELAY
Style=8192

[Attr]
ONV=0,44,SLIDER_MIN,CDELAY

[Attr]
ONV=0,55,SLIDER_MAX,CDELAY

[Comp]
Name=Resistor1
Grid=98,25
Rot=5

[Attr]
ONV=20,-36,PART,R3
Style=8192

[Attr]
ONV=10,-22,VALUE,RDELAY
Style=8192

[Attr]
ONV=8,-71,SLIDER_MAX,4000

[Comp]
Name=Battery1
Grid=104,19
Rot=2

[Attr]
ONV=-32,-23,PART,V4
Style=8192
Height=-16

[Attr]
ONV=-27,-39,VALUE,3
Style=8192
Height=-16

[Attr]
ONV=-28,-79,SLIDER_MAX,3
Height=-16

[Attr]
ONV=0,0,COST,
Height=-16

[Attr]
ONV=0,0,POWER,
Height=-16

[Comp]
Name=Ground
Grid=104,19
Rot=1

[Wire]
Grids=98,26,102,26

[Wire]
Grids=80,27,80,32

[Comp]
Name=Inverter
Grid=102,26
Rot=4

[Attr]
ONV=12,-7,PART,U3
Style=8192

[Attr]
ONV=12,-24,TIMING MODEL,DLY_TTL

[Attr]
ONV=12,-39,I/O MODEL,IO_STD

[Attr]
ONV=12,-54,MNTYMXDLY,0

[Attr]
ONV=12,-69,IO_LEVEL,0

[Attr]
ONV=12,-84,POWER NODE,$G_DPWR

[Attr]
ONV=12,-99,GROUND NODE,$G_DGND

[Wire]
Grids=80,32,109,32

[Wire]
Grids=108,26,109,26

[Wire]
Grids=109,26,109,32

[Wire]
Grids=92,26,93,26

[Wire]
Grids=98,25,98,26

[Wire]
Grids=93,26,98,26

[Comp]
Name=NFI
Grid=98,60
Rot=2

[Attr]
ONV=-28,-33,PART,IA
Style=8192

[Attr]
ONV=-32,21,VALUE,IOUT*(V(E1)>1)
Style=8192

[Attr]
ONV=0,44,DERIVATIVE,Default

[Wire]
Grids=114,26,120,26

[Comp]
Name=Sum
Grid=131,26

[Attr]
ONV=45,5,PART,X1
Style=8192

[Attr]
ONV=45,20,FILE,Sum

[Attr]
ONV=0,11,Param:KA,1

[Attr]
ONV=0,22,Param:KB,1

[Wire]
Grids=123,26,123,32

[Wire]
Grids=123,32,124,32

[Wire]
Grids=135,30,135,32

[Comp]
Name=Delay
Grid=126,32

[Attr]
ONV=4,-24,PART,X2
Style=8192

[Attr]
ONV=0,14,FILE,Delay
Style=8192

[Attr]
ONV=-34,32,Param:DELAY,PERIOD/6
Style=12288

[Comp]
Name=NFV
Grid=114,32
Rot=3

[Attr]
ONV=-31,-28,PART,E8
Style=8192

[Attr]
ONV=-28,-75,VALUE,1.3*(V(D)<1.3)
Style=8192

[Attr]
ONV=0,33,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=114,32
Rot=1

[Comp]
Name=Ground
Grid=100,60
Rot=1

[Comp]
Name=Resistor1
Grid=113,60
Rot=3

[Attr]
ONV=-24,-26,PART,R4
Style=8192

[Attr]
ONV=-38,-41,VALUE,1Meg
Style=8192

[Attr]
ONV=-50,-71,SLIDER_MAX,1e+006

[Wire]
Grids=98,54,100,54

[Wire]
Grids=100,60,113,60

[Wire]
Grids=76,25,80,25

[Wire]
Grids=123,26,131,26

[Wire]
Grids=131,26,134,26

[Wire]
Grids=7,31,15,31

[Comp]
Name=Resistor1
Grid=40,31
Rot=3

[Attr]
ONV=8,-31,PART,R5
Style=8192

[Attr]
ONV=-70,-68,VALUE,(V(INA,INB)>0)*10Meg + 1u
Style=8192

[Attr]
ONV=-50,-71,SLIDER_MAX,1e+006

[Wire]
Grids=25,25,31,25

[Wire]
Grids=132,32,135,32

[Comp]
Name=Delay
Grid=15,55

[Attr]
ONV=22,-34,PART,X4
Style=8192

[Attr]
ONV=0,14,FILE,Delay
Style=8192

[Attr]
ONV=-56,29,Param:DELAY,PERIOD/3
Style=12288

[Wire]
Grids=12,55,13,55

[Wire]
Grids=21,55,24,55

[Comp]
Name=Delay
Grid=27,55

[Attr]
ONV=4,-24,PART,X6
Style=8192

[Attr]
ONV=0,14,FILE,Delay
Style=8192

[Attr]
ONV=-39,30,Param:DELAY,PERIOD/3
Style=12288

[Wire]
Grids=13,55,14,55

[Comp]
Name=Delay
Grid=42,55

[Attr]
ONV=4,-24,PART,X7
Style=8192

[Attr]
ONV=0,14,FILE,Delay
Style=8192

[Attr]
ONV=-47,29,Param:DELAY,PERIOD/6
Style=12288

[Wire]
Grids=48,55,49,55

[Comp]
Name=Delay
Grid=56,55

[Attr]
ONV=4,-24,PART,X8
Style=8192

[Attr]
ONV=0,14,FILE,Delay
Style=8192

[Attr]
ONV=-47,29,Param:DELAY,PERIOD/3
Style=12288

[Wire]
Grids=62,55,68,55

[Comp]
Name=Delay
Grid=70,55

[Attr]
ONV=4,-24,PART,X9
Style=8192

[Attr]
ONV=0,14,FILE,Delay
Style=8192

[Attr]
ONV=-47,29,Param:DELAY,PERIOD/3
Style=12288

[Wire]
Grids=74,55,76,55

[Wire]
Grids=98,60,100,60

[Wire]
Grids=100,54,113,54

[Wire]
Grids=49,55,54,55

[Comp]
Name=NFI
Grid=98,74
Rot=2

[Attr]
ONV=-30,-36,PART,IB
Style=8192

[Attr]
ONV=-29,27,VALUE,IOUT*(V(E2)>1)
Style=8192

[Attr]
ONV=0,44,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=100,74
Rot=1

[Comp]
Name=Resistor1
Grid=113,74
Rot=3

[Attr]
ONV=-24,-26,PART,R6
Style=8192

[Attr]
ONV=-38,-41,VALUE,1Meg
Style=8192

[Attr]
ONV=-50,-71,SLIDER_MAX,1e+006

[Wire]
Grids=98,68,100,68

[Wire]
Grids=100,74,113,74

[Wire]
Grids=98,74,100,74

[Wire]
Grids=100,68,113,68

[Comp]
Name=NFI
Grid=98,89
Rot=2

[Attr]
ONV=-30,-34,PART,IC
Style=8192

[Attr]
ONV=-22,27,VALUE,IOUT*(V(E3)>1)
Style=8192

[Attr]
ONV=0,44,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=100,89
Rot=1

[Comp]
Name=Resistor1
Grid=113,89
Rot=3

[Attr]
ONV=-24,-26,PART,R7
Style=8192

[Attr]
ONV=-38,-41,VALUE,1Meg
Style=8192

[Attr]
ONV=-50,-71,SLIDER_MAX,1e+006

[Wire]
Grids=98,83,100,83

[Wire]
Grids=100,89,113,89

[Wire]
Grids=98,89,100,89

[Wire]
Grids=100,83,113,83

[Comp]
Name=NFI
Grid=123,60
Rot=2

[Attr]
ONV=-30,-37,PART,IAP
Style=8192

[Attr]
ONV=-28,24,VALUE,IOUT*(V(E4)>1)
Style=8192

[Attr]
ONV=0,44,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=125,60
Rot=1

[Comp]
Name=Resistor1
Grid=138,60
Rot=3

[Attr]
ONV=-24,-26,PART,R8
Style=8192

[Attr]
ONV=-38,-41,VALUE,1Meg
Style=8192

[Attr]
ONV=-50,-71,SLIDER_MAX,1e+006

[Wire]
Grids=123,54,125,54

[Wire]
Grids=125,60,138,60

[Wire]
Grids=123,60,125,60

[Comp]
Name=NFI
Grid=123,74
Rot=2

[Attr]
ONV=-39,-28,PART,IBP
Style=8192

[Attr]
ONV=-29,26,VALUE,IOUT*(V(E5)>1)
Style=8192

[Attr]
ONV=0,44,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=125,74
Rot=1

[Comp]
Name=Resistor1
Grid=138,74
Rot=3

[Attr]
ONV=-24,-26,PART,R9
Style=8192

[Attr]
ONV=-38,-41,VALUE,1Meg
Style=8192

[Attr]
ONV=-50,-71,SLIDER_MAX,1e+006

[Wire]
Grids=123,68,125,68

[Wire]
Grids=125,74,138,74

[Wire]
Grids=123,74,125,74

[Wire]
Grids=125,68,138,68

[Comp]
Name=NFI
Grid=123,89
Rot=2

[Attr]
ONV=-38,-30,PART,ICP
Style=8192

[Attr]
ONV=-15,26,VALUE,IOUT*(V(E6)>1)
Style=8192

[Attr]
ONV=0,44,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=125,89
Rot=1

[Comp]
Name=Resistor1
Grid=138,89
Rot=3

[Attr]
ONV=-24,-26,PART,R10
Style=8192

[Attr]
ONV=-38,-41,VALUE,1Meg
Style=8192

[Attr]
ONV=-50,-71,SLIDER_MAX,1e+006

[Wire]
Grids=123,83,126,83

[Wire]
Grids=125,89,138,89

[Wire]
Grids=123,89,125,89

[Wire]
Grids=126,83,138,83

[Wire]
Grids=24,52,24,55

[Wire]
Grids=24,52,40,52

[Wire]
Grids=24,55,25,55

[Wire]
Grids=40,52,40,55

[Wire]
Grids=12,46,12,55

[Wire]
Grids=139,26,139,46

[Wire]
Grids=125,54,138,54

[Wire]
Grids=67,25,68,25

[Wire]
Grids=12,46,139,46

[Wire]
Grids=120,26,123,26

[Node Offsets]

[Condition Offsets]

[Grid Text]
Text=aa
Grid=120,26

[Grid Text]
Text=.PARAMETERS(F0=60,ANGLE=45,IOUT=50M)
Grid=51,10
Height=-18
Color=12

[Grid Text]
Text=E1
Grid=139,26

[Grid Text]
Text=.DEFINE CDELAY 1.5*PW / (.69*RDELAY)
Grid=79,38

[Grid Text]
Text=D
Grid=93,26

[Grid Text]
Text=Comparator
Grid=64,14
Height=-18
FStyle=4
Color=12

[Grid Text]
Text=Six Phase Thyristor Gate Trigger Circuit:þCreates two current pulses of amplitude IOUT for eachþof the six outputs.The first occurs PERIOD*ANGLE/360þseconds after the input signal V(INA,INB) rises past zero,þand the second at PERIOD / 6 seconds later.þþOutputs TA, TB, and TC are separated by 120 degrees.þOutputs TAP occurs at 60 degrees after TA.þOutputs TAP, TBP and TCP are also separated by 120 degrees.þþFiring pattern as per page 142 ofþModern Power Electronics, by Andrzej Trzynadlowski.
Grid=11,98
Height=-21
Color=12
CFill=56
CBorder=30

[Grid Text]
Text=C
Grid=76,25

[Grid Text]
Text=B
Grid=67,25

[Grid Text]
Text=One shot pulse generator
Grid=84,14
Height=-18
FStyle=4
Color=12

[Grid Text]
Text=.DEFINE PW 20U
Grid=79,42

[Grid Text]
Text=Sawtooth generator
Grid=19,14
Height=-18
FStyle=4
Color=12

[Grid Text]
Text=.DEFINE IMAX (.36*F0/MAX(ANGLE,1u))
Grid=79,40

[Grid Text]
Text=A
Grid=25,25

[Grid Text]
Text=INA
Grid=7,25

[Grid Text]
Text=SAW
Grid=56,25
Color=0

[Grid Text]
Text=TA
Grid=100,54

[Grid Text]
Text=.DEFINE RDELAY 4K
Grid=79,36

[Grid Text]
Text=Trigger Macro
Grid=66,3
Height=-19
Color=13

[Grid Text]
Text=Called by other circuits.  Not intended for stand alone analysis.
Grid=49,6
Height=-19
Color=9

[Grid Text]
Text=Pulse doubler
Grid=121,14
Height=-18
FStyle=4
Color=12

[Grid Text]
Text=Output Currents
Grid=107,50
Height=-18
FStyle=4
Color=12

[Grid Text]
Text=INB
Grid=7,31

[Grid Text]
Text=.DEFINE PERIOD (1/F0)
Grid=79,44

[Grid Text]
Text=E2
Grid=21,55

[Grid Text]
Text=E3
Grid=33,55

[Grid Text]
Text=E4
Grid=49,55

[Grid Text]
Text=E5
Grid=62,55

[Grid Text]
Text=E6
Grid=76,55

[Grid Text]
Text=TB
Grid=100,68

[Grid Text]
Text=TC
Grid=100,83

[Grid Text]
Text=TAP
Grid=125,54

[Grid Text]
Text=TBP
Grid=125,68

[Grid Text]
Text=TCP
Grid=126,83

[Grid Text]
Text=Delay Generators
Grid=33,50
Height=-18
FStyle=4
Color=12

[Grid Text]
Text=FIRING ANGLE IS MEASURED WITH RESPECT TO THE ZERO CROSSING POINT OF V(INA,INB).
Grid=7,39
Color=9

[Schematic]
Page 0=0
TabSize 0=320
Page 1=0
TabSize 1=320
Page 2=0
TabSize 2=320
Page 3=0
TabSize 3=320
Splitter.xs=0
Splitter.ys=0
TextQuad=4099
Scale=1
PrinterScale=1
View=304

[Tools]
Pos=Top
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
FLAG=Yes
META=No
INFO=Yes
HELP=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=Yes
GRID=Yes
BORDER=Yes
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FILPX=Yes
FINDCOMP=Yes
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
TOFRONT=Yes
TOBACK=Yes
PAGEADD=Yes
PAGEDEL=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=Yes
COLOR=Yes
FONT=Yes

[Page]
Index=0
Name=Page 1
Scale 0=1.333333333333333
Scale 1=1
Scale 2=1
Scale 3=1
Grid=47,3

[Page]
Index=1
Name=Text
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=2
Name=Models
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=3
Name=Info
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Text Area]
Font=Height=-15,FStyle=0,Color=4,Name=Courier New
Comment Color=8
Background Color=15
Len=0


[Printer]
T.AutoTile=No
T.BlackBorder=No
A.AutoTile=No
A.BlackBorder=No
D.AutoTile=No
D.BlackBorder=No

[TRANSIENT]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[AC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[DC]
AutoTitle=Yes
Grid Weight=1
Grid Pattern=Dot

[Analysis]
Window Placement=0,0, 0,0, 0,0, 0,0,0,0
Window Placement in Probe=0,0, 0,0, 0,0, 0,0,0,0
Num Out Header Left
Num Out Header Center=$MC\n$user\n$company\n$Analysis of $name\n
Num Out Header Right
Num Out Delimiter=32
Analysis Text=Height=-15,FStyle=0,Color=12,Name=Arial
Analysis Grid Color=8
Analysis Graph Background=15
Object Default=Height=-15,FStyle=0,Color=4,Name=Arial
Analysis Window Background=15
NumOut=Height=-15,FStyle=0,Color=4,Name=Courier New
ScaleColor=On
Select Color=9
Select Box Color=4
Cursor Select Color Primary=7
Cursor Select Color Secondary=9
Tracker Intercept=False
Tracker Mouse=True
Tracker Cursor=True
Tracker Foreground=Height=-15,FStyle=0,Color=0,Name=Arial
Tracker Background=11
Data Point Labels Color Fore=Height=-15,FStyle=0,Color=0,Name=Arial
Data Point Labels Color Back=11
AnimateWait=0
AnimateWaitTime=500
Same Y Scales=Yes
T.Save_For_Future=No
A.Save_For_Future=No
D.Save_For_Future=No
T.Reduce_Display=1
T.Reduce_Save=1
A.Reduce_Display=1
A.Reduce_Save=1
D.Reduce_Display=1
D.Reduce_Save=1

[Tools]
Pos=Top
SELECT=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
POLYCLOS=No
SCALE=Yes
CURSOR=Yes
MEASUREH=Yes
MEASUREV=Yes
TAG=Yes
TEXT=Yes
PROPERTY=Yes
START=Yes
STOP=Yes
PAUSE=Yes
DATAPTS=Yes
TOKENS=Yes
RULER=Yes
PLUS=Yes
XAXIS=Yes
YAXIS=Yes
MINORLOG=Yes
BASELINE=Yes
HORIZCUR=Yes
GOTOX=Yes
GOTOY=Yes
GOTOPERF=Yes
GOTOBRNC=Yes
NEXT=Yes
NEXTIN=Yes
PEAK=Yes
VALLEY=Yes
HIGH=Yes
LOW=Yes
INFLECTN=Yes
GHIGH=Yes
GLOW=Yes
BOTTOM=Yes
TOP=Yes
AOUTPUT=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
COLOR=Yes
FONT=Yes

[Monte Carlo Options]
Analysis=Transient
Status=Off
Distribution=Normal
Number of Runs=10

[Monte Carlo Options]
Analysis=AC
Status=Off
Distribution=Normal
Number of Runs=10

[Monte Carlo Options]
Analysis=DC
Status=Off
Distribution=Normal
Number of Runs=10

[Limits]
Analysis=Transient
OPT=120
Horizontal Cursor=False
Temperature Type=Linear

[Limits]
Analysis=AC
OPT=0
Horizontal Cursor=False
Temperature Type=Linear

[Limits]
Analysis=DC
OPT=0
Horizontal Cursor=False
Temperature Type=Linear
Sweep1 type=Auto
Sweep2 type=None

[Optimize]
Format=3

[Optimize]
Analysis=Transient
Method=Standard_Powell

[Optimize]
Analysis=AC
Method=Standard_Powell

[Optimize]
Analysis=DC
Method=Standard_Powell

[Watch]
Format=3

[Watch]
Analysis=Transient
ExprPercentWidth=80

[Watch]
Analysis=AC
ExprPercentWidth=80

[Watch]
Analysis=DC
ExprPercentWidth=80

[DSP]
T.Status=Off
A.Status=Off

[TF]
Input Source
Place Text=False

[SENS]
Multiple=False
Parameter Type=Component
