[Main]
FileType=CIR
Version=8.01
Program=Micro-Cap
Screen=1600,1200
MCAPVersion=1.2.3.4
Key ID=123 456 789
NLCnt=261
TXCnt=30

[shapedef]
Name=Battery
Line=0,0,22,0
Line=22,-3,22,3
Line=26,-7,26,7
Line=26,0,48,0
Current=32,8,16,8

[shapedef]
Name=Resistor
PolyOpen=12 
PolyLine=0,0
PolyLine=0,0
PolyLine=12,0
PolyLine=14,-4
PolyLine=18,4
PolyLine=22,-4
PolyLine=26,4
PolyLine=30,-4
PolyLine=34,4
PolyLine=36,0
PolyLine=48,0
PolyLine=48,0
Current=32,8,16,8

[shapedef]
Name=Capacitor
Line=0,0,22,0
Line=22,-8,22,8
Line=26,-8,26,8
Line=26,0,48,0
Current=32,12,16,12

[shapedef]
Name=Opamp5
Root="Opamp.root",0,-4,0
Root="Plus.root",23,-6,0
Root="Minus.root",23,52,0
Line=32,56,32,34
Line=32,-8,32,13

[shapedef]
Name=Ground
Line=0,0,12,0
Line=12,-8,12,8
Line=18,-4,18,4
Line=24,0,24,0

[shapedef]
Name=Opamp.root
Line=0,48,6,48
Line=0,0,5,0
Line=6,-4,6,52
Line=6,-4,48,24
Line=6,52,48,24
Line=48,24,72,24
Line=10,12,14,12
Line=12,10,12,14
Line=10,36,14,36
Line=4,0,6,0

[shapedef]
Name=Minus.root
Line=-2,0,2,0

[shapedef]
Name=Plus.root
Line=-2,0,2,0
Line=0,-2,0,2

[compdef]
Name=C6_1%
Definition=Resistor
Shape=Resistor
Mask=6272
Label Offset=18,8,9,12
PinCnt=2
Pin="Plus",6,0,-8,-2
Pin="Minus",0,0,-14,-2

[compdef]
Name=LF147
Definition=Opamp
Shape=Opamp5
Mask=4224
memo=Wide bandwidth quad JFET i/p opamp
Label Offset=51,32,-15,46
PinCnt=5
Pin="Plus input",0,0,-30,-3
Pin="Minus input",0,6,-36,17
Pin="VEE",4,7,6,5
Pin="Output",9,3,-13,-4
Pin="VCC",4,-1,6,4

[compdef]
Name=Capacitor
Definition=Capacitor
Shape=Capacitor
Mask=7681
memo=Capacitor
Label Offset=19,8,12,12
PinCnt=2
Pin="Plus",6,0,-3,-5
Pin="Minus",0,0,-14,-5

[compdef]
Name=Ground
Definition=Ground
Shape=Ground
Mask=769
memo=Ground
Label Offset=0,0,0,0
PinCnt=1
Pin="PinA",0,0,-3,-7

[compdef]
Name=Battery
Definition=Battery
Shape=Battery
Mask=5889
memo=Battery
Label Offset=19,7,10,13
PinCnt=2
Pin="Plus",6,0,-4,-5
Pin="Minus",0,0,-10,-5

[Circuit]
Window Placement=2,3, -1,-1, -4,-30, 88,116,1424,840
Default Object=Color=4
Default Object Font=Height=-15,FStyle=0,Color=4,Name=Arial
Default Object Apply Border To Text=No
Default Object Apply Fill To Text=No
WinBackGround Color=15
Select Color=9
Select Box Color=4
Grid Text Color=Height=-12,FStyle=0,Color=1,Name=Arial
Component Color=12
Attribute Text=Height=-12,FStyle=0,Color=2,Name=Arial
Wire Color=2
Pin Connection=Height=-10,FStyle=0,Color=9,Name=Arial
Node Number=Height=-11,FStyle=0,Color=13,Name=Arial
Node Voltage Color=0
Dynamic AC Voltage Color=56
Text Banner Text=Height=-15,FStyle=0,Color=1,Name=Arial
Title Block Background=7
Current=Height=-11,FStyle=0,Color=12,Name=Arial
Power/Condition=Height=-11,FStyle=0,Color=9,Name=Arial
Digital Path Color=9
Title Block=Height=-15,FStyle=0,Color=0,Name=Arial
Digital 0 Color=0
Digital R Color=11
Digital F Color=11
Digital 1 Color=9
Digital X Color=7
Digital Z Color=8
SpiceType=AMBIGUOUS
Block Select Color=41
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=Page $page of $maxpage
TitleBlock One Title=False
Title_Block_Border=False
Title_Block=False

[Comp]
Name=C6_1%
Grid=39,30
Rot=4

[Attr]
ONV=23,-20,PART,R1
Style=8192

[Attr]
ONV=8,12,VALUE,10.10876K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=48,43
Rot=1

[Attr]
ONV=8,11,PART,R2
Style=8192

[Attr]
ONV=8,26,VALUE,7.42328K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=76,35
Rot=4

[Attr]
ONV=44,-44,PART,X1
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=60,17
Rot=4

[Attr]
ONV=19,-23,PART,C1
Style=8192

[Attr]
ONV=13,11,VALUE,24.81714n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=76,28
Rot=6

[Attr]
ONV=-32,-22,PART,R3
Style=8192

[Attr]
ONV=-50,10,VALUE,15.89559K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=76,22
Rot=4

[Attr]
ONV=23,-20,PART,R4
Style=8192

[Attr]
ONV=4,9,VALUE,34.12491K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=Capacitor
Grid=45,39
Rot=2

[Attr]
ONV=-33,-25,PART,C2
Style=8192

[Attr]
ONV=-38,11,VALUE,15.02004n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=58,39
Rot=2

[Attr]
ONV=-32,-25,PART,C3
Style=8192

[Attr]
ONV=-38,11,VALUE,7.51002n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=52,30
Rot=4

[Attr]
ONV=14,-20,PART,R5
Style=8192

[Attr]
ONV=2,12,VALUE,20.21752K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=35,30,39,30

[Wire]
Grids=35,30,35,39

[Wire]
Grids=35,39,39,39

[Wire]
Grids=45,39,48,39

[Wire]
Grids=45,30,48,30

[Wire]
Grids=58,30,62,30

[Wire]
Grids=62,30,62,35

[Wire]
Grids=58,39,62,39

[Wire]
Grids=48,39,48,43

[Wire]
Grids=48,39,52,39

[Comp]
Name=Ground
Grid=48,49
Rot=7

[Comp]
Name=Capacitor
Grid=66,37
Rot=1

[Attr]
ONV=12,12,PART,C4
Style=8192

[Attr]
ONV=7,32,VALUE,5.51492n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=62,35,66,35

[Wire]
Grids=62,35,62,39

[Comp]
Name=Ground
Grid=66,43
Rot=7

[Comp]
Name=C6_1%
Grid=76,37
Rot=1

[Attr]
ONV=8,11,PART,R6
Style=8192

[Attr]
ONV=8,26,VALUE,33.40477K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=66,35,66,37

[Wire]
Grids=76,35,76,37

[Comp]
Name=Ground
Grid=76,43
Rot=7

[Wire]
Grids=76,22,76,28

[Wire]
Grids=82,22,85,22

[Wire]
Grids=85,22,85,30

[Comp]
Name=Ground
Grid=70,28
Rot=2

[Wire]
Grids=66,17,85,17

[Wire]
Grids=85,17,85,22

[Wire]
Grids=48,17,60,17

[Wire]
Grids=48,17,48,30

[Wire]
Grids=48,30,52,30

[Wire]
Grids=76,28,76,29

[Wire]
Grids=66,35,76,35

[Wire]
Grids=33,30,35,30

[Wire]
Grids=85,30,90,30

[Wire]
Grids=85,30,85,32

[Comp]
Name=C6_1%
Grid=94,30
Rot=4

[Attr]
ONV=23,-20,PART,R8
Style=8192

[Attr]
ONV=8,12,VALUE,11.13492K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=103,43
Rot=1

[Attr]
ONV=8,11,PART,R9
Style=8192

[Attr]
ONV=8,26,VALUE,6.73917K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=131,35
Rot=4

[Attr]
ONV=44,-44,PART,X2
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=115,17
Rot=4

[Attr]
ONV=19,-23,PART,C5
Style=8192

[Attr]
ONV=13,11,VALUE,20.45375n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=131,28
Rot=6

[Attr]
ONV=-32,-22,PART,R10
Style=8192

[Attr]
ONV=-50,10,VALUE,15.89559K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=131,22
Rot=4

[Attr]
ONV=23,-20,PART,R11
Style=8192

[Attr]
ONV=4,9,VALUE,39.2026K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=Capacitor
Grid=100,39
Rot=2

[Attr]
ONV=-33,-25,PART,C6
Style=8192

[Attr]
ONV=-38,11,VALUE,15.02004n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=113,39
Rot=2

[Attr]
ONV=-32,-25,PART,C7
Style=8192

[Attr]
ONV=-38,11,VALUE,7.51002n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=107,30
Rot=4

[Attr]
ONV=14,-20,PART,R12
Style=8192

[Attr]
ONV=2,12,VALUE,22.26985K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=90,30,94,30

[Wire]
Grids=90,30,90,39

[Wire]
Grids=90,39,94,39

[Wire]
Grids=100,39,103,39

[Wire]
Grids=100,30,103,30

[Wire]
Grids=113,30,117,30

[Wire]
Grids=117,30,117,35

[Wire]
Grids=113,39,117,39

[Wire]
Grids=103,39,103,43

[Wire]
Grids=103,39,107,39

[Comp]
Name=Ground
Grid=103,49
Rot=7

[Comp]
Name=Capacitor
Grid=121,37
Rot=1

[Attr]
ONV=12,12,PART,C8
Style=8192

[Attr]
ONV=7,32,VALUE,4.54528n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=117,35,121,35

[Wire]
Grids=117,35,117,39

[Comp]
Name=Ground
Grid=121,43
Rot=7

[Comp]
Name=C6_1%
Grid=131,37
Rot=1

[Attr]
ONV=8,11,PART,R13
Style=8192

[Attr]
ONV=8,26,VALUE,30.32628K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=121,35,121,37

[Wire]
Grids=131,35,131,37

[Comp]
Name=Ground
Grid=131,43
Rot=7

[Wire]
Grids=131,22,131,28

[Wire]
Grids=137,22,140,22

[Wire]
Grids=140,22,140,30

[Comp]
Name=Ground
Grid=125,28
Rot=2

[Wire]
Grids=121,17,140,17

[Wire]
Grids=140,17,140,22

[Wire]
Grids=103,17,115,17

[Wire]
Grids=103,17,103,30

[Wire]
Grids=103,30,107,30

[Wire]
Grids=131,28,131,29

[Wire]
Grids=121,35,131,35

[Wire]
Grids=140,30,145,30

[Wire]
Grids=140,30,140,32

[Comp]
Name=C6_1%
Grid=149,30
Rot=4

[Attr]
ONV=23,-20,PART,R15
Style=8192

[Attr]
ONV=8,12,VALUE,10.23475K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=158,43
Rot=1

[Attr]
ONV=8,11,PART,R16
Style=8192

[Attr]
ONV=8,26,VALUE,7.32397K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=186,35
Rot=4

[Attr]
ONV=44,-44,PART,X3
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=170,17
Rot=4

[Attr]
ONV=19,-23,PART,C9
Style=8192

[Attr]
ONV=13,11,VALUE,24.1968n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=186,28
Rot=6

[Attr]
ONV=-32,-22,PART,R17
Style=8192

[Attr]
ONV=-50,10,VALUE,15.89559K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=186,22
Rot=4

[Attr]
ONV=23,-20,PART,R18
Style=8192

[Attr]
ONV=4,9,VALUE,33.82986K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=Capacitor
Grid=155,39
Rot=2

[Attr]
ONV=-33,-25,PART,C10
Style=8192

[Attr]
ONV=-38,11,VALUE,15.02817n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=168,39
Rot=2

[Attr]
ONV=-32,-25,PART,C11
Style=8192

[Attr]
ONV=-38,11,VALUE,7.51408n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=162,30
Rot=4

[Attr]
ONV=14,-20,PART,R19
Style=8192

[Attr]
ONV=2,12,VALUE,20.4695K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=145,30,149,30

[Wire]
Grids=145,30,145,39

[Wire]
Grids=145,39,149,39

[Wire]
Grids=155,39,158,39

[Wire]
Grids=155,30,158,30

[Wire]
Grids=168,30,172,30

[Wire]
Grids=172,30,172,35

[Wire]
Grids=168,39,172,39

[Wire]
Grids=158,39,158,43

[Wire]
Grids=158,39,162,39

[Comp]
Name=Ground
Grid=158,49
Rot=7

[Comp]
Name=Capacitor
Grid=176,37
Rot=1

[Attr]
ONV=12,12,PART,C12
Style=8192

[Attr]
ONV=7,32,VALUE,5.37707n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=172,35,176,35

[Wire]
Grids=172,35,172,39

[Comp]
Name=Ground
Grid=176,43
Rot=7

[Comp]
Name=C6_1%
Grid=186,37
Rot=1

[Attr]
ONV=8,11,PART,R20
Style=8192

[Attr]
ONV=8,26,VALUE,32.95787K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=176,35,176,37

[Wire]
Grids=186,35,186,37

[Comp]
Name=Ground
Grid=186,43
Rot=7

[Wire]
Grids=186,22,186,28

[Wire]
Grids=192,22,195,22

[Wire]
Grids=195,22,195,30

[Comp]
Name=Ground
Grid=180,28
Rot=2

[Wire]
Grids=176,17,195,17

[Wire]
Grids=195,17,195,22

[Wire]
Grids=158,17,170,17

[Wire]
Grids=158,17,158,30

[Wire]
Grids=158,30,162,30

[Wire]
Grids=186,28,186,29

[Wire]
Grids=176,35,186,35

[Wire]
Grids=195,30,200,30

[Wire]
Grids=195,30,195,32

[Comp]
Name=C6_1%
Grid=204,30
Rot=4

[Attr]
ONV=23,-20,PART,R22
Style=8192

[Attr]
ONV=8,12,VALUE,10.98596K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=213,43
Rot=1

[Attr]
ONV=8,11,PART,R23
Style=8192

[Attr]
ONV=8,26,VALUE,6.82317K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=241,35
Rot=4

[Attr]
ONV=44,-44,PART,X4
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=225,17
Rot=4

[Attr]
ONV=19,-23,PART,C13
Style=8192

[Attr]
ONV=13,11,VALUE,21.00085n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=241,28
Rot=6

[Attr]
ONV=-32,-22,PART,R24
Style=8192

[Attr]
ONV=-50,10,VALUE,15.89559K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=241,22
Rot=4

[Attr]
ONV=23,-20,PART,R25
Style=8192

[Attr]
ONV=4,9,VALUE,37.47958K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=Capacitor
Grid=210,39
Rot=2

[Attr]
ONV=-33,-25,PART,C14
Style=8192

[Attr]
ONV=-38,11,VALUE,15.02817n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=223,39
Rot=2

[Attr]
ONV=-32,-25,PART,C15
Style=8192

[Attr]
ONV=-38,11,VALUE,7.51408n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=217,30
Rot=4

[Attr]
ONV=14,-20,PART,R26
Style=8192

[Attr]
ONV=2,12,VALUE,21.97191K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=200,30,204,30

[Wire]
Grids=200,30,200,39

[Wire]
Grids=200,39,204,39

[Wire]
Grids=210,39,213,39

[Wire]
Grids=210,30,213,30

[Wire]
Grids=223,30,227,30

[Wire]
Grids=227,30,227,35

[Wire]
Grids=223,39,227,39

[Wire]
Grids=213,39,213,43

[Wire]
Grids=213,39,217,39

[Comp]
Name=Ground
Grid=213,49
Rot=7

[Comp]
Name=Capacitor
Grid=231,37
Rot=1

[Attr]
ONV=12,12,PART,C16
Style=8192

[Attr]
ONV=7,32,VALUE,4.66685n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=227,35,231,35

[Wire]
Grids=227,35,227,39

[Comp]
Name=Ground
Grid=231,43
Rot=7

[Comp]
Name=C6_1%
Grid=241,37
Rot=1

[Attr]
ONV=8,11,PART,R27
Style=8192

[Attr]
ONV=8,26,VALUE,30.70426K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=231,35,231,37

[Wire]
Grids=241,35,241,37

[Comp]
Name=Ground
Grid=241,43
Rot=7

[Wire]
Grids=241,22,241,28

[Wire]
Grids=247,22,250,22

[Wire]
Grids=250,22,250,30

[Comp]
Name=Ground
Grid=235,28
Rot=2

[Wire]
Grids=231,17,250,17

[Wire]
Grids=250,17,250,22

[Wire]
Grids=213,17,225,17

[Wire]
Grids=213,17,213,30

[Wire]
Grids=213,30,217,30

[Wire]
Grids=241,28,241,29

[Wire]
Grids=231,35,241,35

[Wire]
Grids=250,30,255,30

[Wire]
Grids=250,30,250,32

[Comp]
Name=C6_1%
Grid=259,30
Rot=4

[Attr]
ONV=23,-20,PART,R29
Style=8192

[Attr]
ONV=8,12,VALUE,10.46136K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=268,43
Rot=1

[Attr]
ONV=8,11,PART,R30
Style=8192

[Attr]
ONV=8,26,VALUE,7.15755K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=296,35
Rot=4

[Attr]
ONV=44,-44,PART,X5
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=280,17
Rot=4

[Attr]
ONV=19,-23,PART,C17
Style=8192

[Attr]
ONV=13,11,VALUE,23.1473n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=296,28
Rot=6

[Attr]
ONV=-32,-22,PART,R31
Style=8192

[Attr]
ONV=-50,10,VALUE,15.89559K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=296,22
Rot=4

[Attr]
ONV=23,-20,PART,R32
Style=8192

[Attr]
ONV=4,9,VALUE,34.38788K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=Capacitor
Grid=265,39
Rot=2

[Attr]
ONV=-33,-25,PART,C18
Style=8192

[Attr]
ONV=-38,11,VALUE,15.03633n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=278,39
Rot=2

[Attr]
ONV=-32,-25,PART,C19
Style=8192

[Attr]
ONV=-38,11,VALUE,7.51816n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=272,30
Rot=4

[Attr]
ONV=14,-20,PART,R33
Style=8192

[Attr]
ONV=2,12,VALUE,20.92272K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=255,30,259,30

[Wire]
Grids=255,30,255,39

[Wire]
Grids=255,39,259,39

[Wire]
Grids=265,39,268,39

[Wire]
Grids=265,30,268,30

[Wire]
Grids=278,30,282,30

[Wire]
Grids=282,30,282,35

[Wire]
Grids=278,39,282,39

[Wire]
Grids=268,39,268,43

[Wire]
Grids=268,39,272,39

[Comp]
Name=Ground
Grid=268,49
Rot=7

[Comp]
Name=Capacitor
Grid=286,37
Rot=1

[Attr]
ONV=12,12,PART,C20
Style=8192

[Attr]
ONV=7,32,VALUE,5.14384n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=282,35,286,35

[Wire]
Grids=282,35,282,39

[Comp]
Name=Ground
Grid=286,43
Rot=7

[Comp]
Name=C6_1%
Grid=296,37
Rot=1

[Attr]
ONV=8,11,PART,R34
Style=8192

[Attr]
ONV=8,26,VALUE,32.20897K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=286,35,286,37

[Wire]
Grids=296,35,296,37

[Comp]
Name=Ground
Grid=296,43
Rot=7

[Wire]
Grids=296,22,296,28

[Wire]
Grids=302,22,305,22

[Wire]
Grids=305,22,305,30

[Comp]
Name=Ground
Grid=290,28
Rot=2

[Wire]
Grids=286,17,305,17

[Wire]
Grids=305,17,305,22

[Wire]
Grids=268,17,280,17

[Wire]
Grids=268,17,268,30

[Wire]
Grids=268,30,272,30

[Wire]
Grids=296,28,296,29

[Wire]
Grids=286,35,296,35

[Wire]
Grids=305,30,310,30

[Wire]
Grids=305,30,305,32

[Comp]
Name=C6_1%
Grid=314,30
Rot=4

[Attr]
ONV=23,-20,PART,R36
Style=8192

[Attr]
ONV=8,12,VALUE,10.73632K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=323,43
Rot=1

[Attr]
ONV=8,11,PART,R37
Style=8192

[Attr]
ONV=8,26,VALUE,6.97424K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=LF147
Grid=351,35
Rot=4

[Attr]
ONV=44,-44,PART,X6
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=Capacitor
Grid=335,17
Rot=4

[Attr]
ONV=19,-23,PART,C21
Style=8192

[Attr]
ONV=13,11,VALUE,21.97687n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=351,28
Rot=6

[Attr]
ONV=-32,-22,PART,R38
Style=8192

[Attr]
ONV=-50,10,VALUE,15.89559K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=351,22
Rot=4

[Attr]
ONV=23,-20,PART,R39
Style=8192

[Attr]
ONV=4,9,VALUE,35.7095K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=Capacitor
Grid=320,39
Rot=2

[Attr]
ONV=-33,-25,PART,C22
Style=8192

[Attr]
ONV=-38,11,VALUE,15.03633n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=Capacitor
Grid=333,39
Rot=2

[Attr]
ONV=-32,-25,PART,C23
Style=8192

[Attr]
ONV=-38,11,VALUE,7.51816n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Comp]
Name=C6_1%
Grid=327,30
Rot=4

[Attr]
ONV=14,-20,PART,R40
Style=8192

[Attr]
ONV=2,12,VALUE,21.47264K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=310,30,314,30

[Wire]
Grids=310,30,310,39

[Wire]
Grids=310,39,314,39

[Wire]
Grids=320,39,323,39

[Wire]
Grids=320,30,323,30

[Wire]
Grids=333,30,337,30

[Wire]
Grids=337,30,337,35

[Wire]
Grids=333,39,337,39

[Wire]
Grids=323,39,323,43

[Wire]
Grids=323,39,327,39

[Comp]
Name=Ground
Grid=323,49
Rot=7

[Comp]
Name=Capacitor
Grid=341,37
Rot=1

[Attr]
ONV=12,12,PART,C24
Style=8192

[Attr]
ONV=7,32,VALUE,4.88375n
Style=8192

[Attr]
ONV=0,33,MODEL,CM1

[Wire]
Grids=337,35,341,35

[Wire]
Grids=337,35,337,39

[Comp]
Name=Ground
Grid=341,43
Rot=7

[Comp]
Name=C6_1%
Grid=351,37
Rot=1

[Attr]
ONV=8,11,PART,R41
Style=8192

[Attr]
ONV=8,26,VALUE,31.38408K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Wire]
Grids=341,35,341,37

[Wire]
Grids=351,35,351,37

[Comp]
Name=Ground
Grid=351,43
Rot=7

[Wire]
Grids=351,22,351,28

[Wire]
Grids=357,22,360,22

[Wire]
Grids=360,22,360,30

[Comp]
Name=Ground
Grid=345,28
Rot=2

[Wire]
Grids=341,17,360,17

[Wire]
Grids=360,17,360,22

[Wire]
Grids=323,17,335,17

[Wire]
Grids=323,17,323,30

[Wire]
Grids=323,30,327,30

[Wire]
Grids=351,28,351,29

[Wire]
Grids=341,35,351,35

[Wire]
Grids=360,30,367,30

[Wire]
Grids=360,30,360,32

[Comp]
Name=Battery
Grid=6,11
Rot=3

[Attr]
ONV=-24,-28,PART,V3
Style=8192

[Attr]
ONV=-24,-43,VALUE,15
Style=8192

[Comp]
Name=Ground
Grid=6,11
Rot=7

[Comp]
Name=Battery
Grid=14,5
Rot=7

[Attr]
ONV=-24,13,PART,V4
Style=8192

[Attr]
ONV=-24,28,VALUE,15
Style=8192

[Comp]
Name=Ground
Grid=14,11
Rot=7

[Comp]
Name=LF147
Grid=373,36
Rot=4

[Attr]
ONV=44,-44,PART,X7
Style=8192

[Attr]
ONV=0,11,MODEL,$IDEAL

[Comp]
Name=C6_1%
Grid=380,23
Rot=6

[Attr]
ONV=-35,-23,PART,R43
Style=8192

[Attr]
ONV=-50,10,VALUE,867.81538
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=C6_1%
Grid=373,30
Rot=2

[Attr]
ONV=-34,-21,PART,R44
Style=8192

[Attr]
ONV=-47,13,VALUE,15.89559K
Style=8192

[Attr]
ONV=0,33,MODEL,RM1

[Comp]
Name=Ground
Grid=373,36
Rot=1

[Wire]
Grids=382,23,382,30

[Wire]
Grids=380,23,382,23

[Wire]
Grids=373,23,374,23

[Wire]
Grids=373,23,373,30

[Wire]
Grids=382,30,384,30

[Wire]
Grids=382,30,382,33

[Grid Text]
Text="VM"
Grid=80,28
CBorder=NONE

[Grid Text]
Text="VP"
Grid=80,36
CBorder=NONE

[Grid Text]
Text="Stage 1:Sallen-KeyþF1 = (1)*(U*U+1)/(U*U+0.024663*U+0.90784)þPoles = -0.012331, -0.95273jþZeros = 0.0 , 0j"
Grid=44,59
CBorder=NONE

[Grid Text]
Text="VM"
Grid=135,28
CBorder=NONE

[Grid Text]
Text="VP"
Grid=135,36
CBorder=NONE

[Grid Text]
Text="Stage 2:Sallen-KeyþF2 = (1)*(U*U+1)/(U*U+0.027166*U+1.1015)þPoles = -0.013583, -1.0494jþZeros = 0.0 , 0j"
Grid=100,59
CBorder=NONE

[Grid Text]
Text="VM"
Grid=190,28
CBorder=NONE

[Grid Text]
Text="VP"
Grid=190,36
CBorder=NONE

[Grid Text]
Text="Stage 3:Sallen-KeyþF3 = (1)*(U*U+1)/(U*U+0.068293*U+0.93162)þPoles = -0.034146, -0.9646jþZeros = 0.0 , 0j"
Grid=154,59
CBorder=NONE

[Grid Text]
Text="VM"
Grid=245,28
CBorder=NONE

[Grid Text]
Text="VP"
Grid=245,36
CBorder=NONE

[Grid Text]
Text="Stage 4:Sallen-KeyþF4 = (1)*(U*U+1)/(U*U+0.073305*U+1.0734)þPoles = -0.036653, -1.0354jþZeros = 0.0 , 0j"
Grid=210,59
CBorder=NONE

[Grid Text]
Text="VM"
Grid=300,28
CBorder=NONE

[Grid Text]
Text="VP"
Grid=300,36
CBorder=NONE

[Grid Text]
Text="Stage 5:Sallen-KeyþF5 = (1)*(U*U+1)/(U*U+0.095459*U+0.97439)þPoles = -0.04773, -0.98596jþZeros = 0.0 , 0j"
Grid=264,59
CBorder=NONE

[Grid Text]
Text="VM"
Grid=355,28
CBorder=NONE

[Grid Text]
Text="VP"
Grid=355,36
CBorder=NONE

[Grid Text]
Text="Stage 6:Sallen-KeyþF6 = (1)*(U*U+1)/(U*U+0.097968*U+1.0263)þPoles = -0.048984, -1.0119jþZeros = 0.0 , 0j"
Grid=320,59
CBorder=NONE

[Grid Text]
Text="VM"
Grid=14,5
CBorder=NONE

[Grid Text]
Text="VP"
Grid=6,5
CBorder=NONE

[Grid Text]
Text="In"
Grid=33,30
CBorder=NONE

[Grid Text]
Text="Notch Butterworth Sallen-KeyþGain=0dB Center Frequency=1000Hz Ripple=1dB Order=6 Q=10þImpedance Scale Factor=1, and OPAMP model=$IDEAL"
Grid=20,6
Color=12
CFill=7
CBorder=0

[Grid Text]
Text="LP = Ideal low-pass response based upon choice of filter type and response. þBR = Ideal notch response transformed from the low pass response.  þThe circuit above is designed to match this transfer response. "
Grid=33,68
CBorder=NONE

[Grid Text]
Text=".define U (S/(2*PI*998.75))"
Grid=33,71
CBorder=NONE

[Grid Text]
Text=".define LP þ1/(U*U+0.51764*U+1)*þ1/(U*U+1.4142*U+1)*þ1/(U*U+1.9319*U+1)*þ1 "
Grid=33,82
CBorder=NONE

[Grid Text]
Text=".define BRþ(1*U*U+1)/(U*U+0.024663*U+0.90784)*þ(1*U*U+1)/(U*U+0.027166*U+1.1015)*þ(1*U*U+1)/(U*U+0.068293*U+0.93162)*þ(1*U*U+1)/(U*U+0.073305*U+1.0734)*þ(1*U*U+1)/(U*U+0.095459*U+0.97439)*þ(1*U*U+1)/(U*U+0.097968*U+1.0263)"
Grid=33,97
CBorder=NONE

[Grid Text]
Text="VM"
Grid=377,29
CBorder=NONE

[Grid Text]
Text="VP"
Grid=377,37
CBorder=NONE

[Grid Text]
Text="Out"
Grid=384,30
CBorder=NONE

[Grid Text]
Text="Stage 7:Gain Adjustment stageþGain = 0.0545947þ"
Grid=363,55
CBorder=NONE

[Schematic]
Page 0=0
TabSize 0=340
Page 1=0
TabSize 1=340
Page 2=0
TabSize 2=340
Page 3=0
TabSize 3=340
Splitter.xs=0
Splitter.ys=0
TextQuad=4099
Scale=1
PrinterScale=1
View=304
GridUser=10

[Tools]
Pos=Top
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
LEFTBRK=No
RIGHTBRK=No
BOTHBRK=No
FLAG=Yes
META=No
INFO=Yes
HELP=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=Yes
GRID=Yes
BORDER=Yes
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FILPX=Yes
FINDCOMP=Yes
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
TOFRONT=Yes
TOBACK=Yes
PAGEADD=Yes
PAGEDEL=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=Yes
COLOR=Yes
FONT=Yes

[Page]
Index=0
Print=True
Name=Main
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=1
Type=Text
Print=False
Name=Text
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=2
Type=Text
Print=False
Name=Models
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Page]
Index=3
Type=Info
Print=False
Name=Info
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=0,0

[Text Area]
Page=1
Font=Height=-15,FStyle=0,Color=4,Name=Courier New
Comment Color=8
Background Color=15
Len=0


[Text Area]
Page=2
Font=Height=-15,FStyle=0,Color=4,Name=Courier New
Comment Color=8
Background Color=15
Len=114
.MODEL $IDEAL OPA (Level=1 A=1E8 RoutAC=.5m RoutDC=1m)
.MODEL RM1 RES (R=1 LOT=1%)
.MODEL CM1 CAP (C=1 LOT=1%)


[Limits]
Analysis=DynamicAC
FirstValueDisplay=Mag
SecondValueDisplay=PhaseDeg
PlaceText=True

[Limits]
Analysis=DynamicDC
PlaceText=True

[Optimize]
Format=3
